Functions
FLAG_Management
Peripheral Driver » LL Driver » RTC » Functions
Collaboration diagram for FLAG_Management:

## Functions
__STATIC_INLINE uint32_t | ll_rtc_is_active_flag_alarm (rtc_regs_t *RTCx)
| Indicate if the RTC alarm event flag is set or not. More...
__STATIC_INLINE uint32_t | ll_rtc_is_active_flag_wrap (rtc_regs_t *RTCx)
| Indicate if the RTC wrap event flag is set or not. More...
__STATIC_INLINE uint32_t | ll_rtc_is_active_flag_tick (rtc_regs_t *RTCx)
| Indicate if the RTC tick event flag is set or not. More...
__STATIC_INLINE void | ll_rtc_clear_flag_alarm (rtc_regs_t *RTCx)
| Clear RTC alarm interrupt flag. More...
__STATIC_INLINE void | ll_rtc_clear_flag_wrap (rtc_regs_t *RTCx)
| Clear RTC wrap interrupt flag. More...
__STATIC_INLINE void | ll_rtc_clear_flag_tick (rtc_regs_t *RTCx)
| Clear RTC tick interrupt flag. More...
__STATIC_INLINE void | ll_rtc_clear_it_event (rtc_regs_t *RTCx)
__STATIC_INLINE void | ll_rtc_clear_tick_it_event (rtc_regs_t *RTCx)
__STATIC_INLINE void | ll_rtc_it_enable_wakeup_by_rtc (rtc_regs_t *RTCx)
| Enable RTC alarm wakeup interrupt. More...
__STATIC_INLINE void | ll_rtc_it_disable_wakeup_by_rtc (rtc_regs_t *RTCx)
| Disable RTC alarm wakeup interrupt. More...

## Detailed Description

## Function Documentation

## ◆ ll_rtc_clear_flag_alarm()

__STATIC_INLINE void ll_rtc_clear_flag_alarm | ( | rtc_regs_t * | RTCx | ) |

Clear RTC alarm interrupt flag.

Register | BitsName
--- | ---
SLP_EVENT | RTC_TIMER_ALARM

Return values

  None |

Definition at line 756 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_clear_flag_tick()

__STATIC_INLINE void ll_rtc_clear_flag_tick | ( | rtc_regs_t * | RTCx | ) |

Clear RTC tick interrupt flag.

Register | BitsName
--- | ---
SLP_EVENT | RTC_TIMER_WRAP

Return values

  None |

Definition at line 785 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_clear_flag_wrap()

__STATIC_INLINE void ll_rtc_clear_flag_wrap | ( | rtc_regs_t * | RTCx | ) |

Clear RTC wrap interrupt flag.

Register | BitsName
--- | ---
RTC_INT_STAT | RTC_TICK

Return values

  None |

Definition at line 770 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_clear_it_event()

__STATIC_INLINE void ll_rtc_clear_it_event | ( | rtc_regs_t * | RTCx | ) |

Definition at line 790 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_clear_tick_it_event()

__STATIC_INLINE void ll_rtc_clear_tick_it_event | ( | rtc_regs_t * | RTCx | ) |

Definition at line 802 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_is_active_flag_alarm()

__STATIC_INLINE uint32_t ll_rtc_is_active_flag_alarm | ( | rtc_regs_t * | RTCx | ) |

Indicate if the RTC alarm event flag is set or not.

Note
  This bit is set by hardware when the counter has reached alarm value. It can be cleared by writing 0 to this bit.

Register | BitsName
--- | ---
SLP_EVENT | RTC_TIMER_ALARM

Return values

  State | of bit (1 or 0).

Definition at line 710 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_is_active_flag_tick()

__STATIC_INLINE uint32_t ll_rtc_is_active_flag_tick | ( | rtc_regs_t * | RTCx | ) |

Indicate if the RTC tick event flag is set or not.

Note
  This bit is set by hardware when the counter has reached to 0. It can be cleared by writing 1 to this bit.

Register | BitsName
--- | ---
RTC_INT_STAT | TICK_INT_STAT

Return values

  State | of bit (1 or 0).

Definition at line 742 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_is_active_flag_wrap()

__STATIC_INLINE uint32_t ll_rtc_is_active_flag_wrap | ( | rtc_regs_t * | RTCx | ) |

Indicate if the RTC wrap event flag is set or not.

Note
  This bit is set by hardware when the counter has overflow. It can be cleared by writing 0 to this bit.

Register | BitsName
--- | ---
SLP_EVENT | CALENDAR_TIMER_WRAP

Return values

  State | of bit (1 or 0).

Definition at line 726 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_it_disable_wakeup_by_rtc()

__STATIC_INLINE void ll_rtc_it_disable_wakeup_by_rtc | ( | rtc_regs_t * | RTCx | ) |

Disable RTC alarm wakeup interrupt.

Register | BitsName
--- | ---
AON_MISC | MCU_WAKEUP_CTRL

Return values

  None |

Definition at line 844 of file gr55xx_ll_rtc.h.

## ◆ ll_rtc_it_enable_wakeup_by_rtc()

__STATIC_INLINE void ll_rtc_it_enable_wakeup_by_rtc | ( | rtc_regs_t * | RTCx | ) |

Enable RTC alarm wakeup interrupt.

Register | BitsName
--- | ---
AON_MISC | MCU_WAKEUP_CTRL

Return values

  None |

Definition at line 823 of file gr55xx_ll_rtc.h.