Macros
data frame size in xip, take effect when enable DFS_HC
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for data frame size in xip, take effect when enable DFS_HC:

## Macros
#define | QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_CONCURRENT_XIP_DFS_BYTE
| Set data frame size as byte. More...
#define | QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD
| Set data frame size as halfword. More...
#define | QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_CONCURRENT_XIP_DFS_WORD
| Set data frame size as word. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_DFS_BYTE

#define QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_CONCURRENT_XIP_DFS_BYTE

Set data frame size as byte.

Definition at line 583 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_DFS_HALFWORD

#define QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD

Set data frame size as halfword.

Definition at line 584 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_DFS_WORD

#define QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_CONCURRENT_XIP_DFS_WORD

Set data frame size as word.

Definition at line 585 of file gr55xx_hal_qspi.h.