Macros
Master Addressing Mode
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants
Collaboration diagram for Master Addressing Mode:

## Macros
#define | LL_I2C_ADDRESSING_MODE_7BIT 0x00000000U
| Master operates in 7-bit addressing mode. More...
#define | LL_I2C_ADDRESSING_MODE_10BIT I2C_CTRL_ADDR_BIT_M
| Master operates in 10-bit addressing mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_ADDRESSING_MODE_10BIT

#define LL_I2C_ADDRESSING_MODE_10BIT I2C_CTRL_ADDR_BIT_M

Master operates in 10-bit addressing mode.

Definition at line 173 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_ADDRESSING_MODE_7BIT

#define LL_I2C_ADDRESSING_MODE_7BIT 0x00000000U

Master operates in 7-bit addressing mode.

Definition at line 172 of file gr55xx_ll_i2c.h.