Public Attributes | List of all members
dma_gather_config Struct Reference
Peripheral Driver » HAL Driver » DMA » Structures » DMA Configuration

LL DMA gather config definition. More...

`#include <gr55xx_hal_dma.h>`

## Public Attributes
uint32_t | src_gather_en
| Specifies the channel source gather function enable. More...
uint32_t | src_sgi
| Specifies the channel source gather interval. More...
uint32_t | src_sgc
| Specifies the channel source gather count. More...

## Detailed Description

LL DMA gather config definition.

Definition at line 180 of file gr55xx_hal_dma.h.

## Member Data Documentation

## ◆ src_gather_en

uint32_t dma_gather_config::src_gather_en

Specifies the channel source gather function enable.

This parameter can be a value of Source Gather Enable.

Definition at line 183 of file gr55xx_hal_dma.h.

## ◆ src_sgc

uint32_t dma_gather_config::src_sgc

Specifies the channel source gather count.

This parameter can be a value between Min_Data = 0 and Max_Data = 0xFFF.

Definition at line 189 of file gr55xx_hal_dma.h.

## ◆ src_sgi

uint32_t dma_gather_config::src_sgi

Specifies the channel source gather interval.

This parameter can be a value between Min_Data = 0 and Max_Data = 0xFFFFF.

Definition at line 186 of file gr55xx_hal_dma.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_dma.h