Macros
Common Write and read registers Macros
Peripheral Driver » LL Driver » AES » Defines » AES Exported Macros
Collaboration diagram for Common Write and read registers Macros:

## Macros
#define | LL_AES_WriteReg(__INSTANCE__, __REG__, __VALUE__) WRITE_REG(__INSTANCE__->__REG__, (__VALUE__))
| Write a value in AES register. More...
#define | LL_AES_ReadReg(__INSTANCE__, __REG__) READ_REG(__INSTANCE__->__REG__)
| Read a value in AES register. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AES_ReadReg

#define LL_AES_ReadReg | ( |  | __INSTANCE__,
|  |  | __REG__
| ) |  | READ_REG(__INSTANCE__->__REG__)

Read a value in AES register.

Parameters

  <strong>INSTANCE</strong> | AES Instance
  <strong>REG</strong> | Register to be read

Return values

  Register | value

Definition at line 168 of file gr55xx_ll_aes.h.

## ◆ LL_AES_WriteReg

#define LL_AES_WriteReg | ( |  | __INSTANCE__,
|  |  | __REG__,
|  |  | __VALUE__
| ) |  | WRITE_REG(__INSTANCE__->__REG__, (__VALUE__))

Write a value in AES register.

Parameters

  <strong>INSTANCE</strong> | AES Instance
  <strong>REG</strong> | Register to be written
  <strong>VALUE</strong> | Value to be written in the register

Return values

  None |

Definition at line 160 of file gr55xx_ll_aes.h.