Public Attributes | List of all members
_ll_aes_init Struct Reference
Peripheral Driver » LL Driver » AES » Structures » AES Exported Init structures

LL AES Init Structure definition. More...

`#include <gr55xx_ll_aes.h>`

## Public Attributes
uint32_t | key_size
| 128, 192 or 256-bit key length. More...
uint32_t * | p_key
| Encryption/Decryption Key. More...
uint32_t * | p_init_vector
| Initialization Vector used for CBC modes. More...
uint32_t * | p_seed
| Random seeds. More...

## Detailed Description

LL AES Init Structure definition.

Definition at line 75 of file gr55xx_ll_aes.h.

## Member Data Documentation

## ◆ key_size

uint32_t _ll_aes_init::key_size

128, 192 or 256-bit key length.

This parameter can be a value of Key Size

Definition at line 77 of file gr55xx_ll_aes.h.

## ◆ p_init_vector

uint32_t* _ll_aes_init::p_init_vector

Initialization Vector used for CBC modes.

Definition at line 82 of file gr55xx_ll_aes.h.

## ◆ p_key

uint32_t* _ll_aes_init::p_key

Encryption/Decryption Key.

Definition at line 80 of file gr55xx_ll_aes.h.

## ◆ p_seed

uint32_t* _ll_aes_init::p_seed

Random seeds.

Definition at line 84 of file gr55xx_ll_aes.h.

The documentation for this struct was generated from the following file:

- gr55xx_ll_aes.h