Macros
Datawidth
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for Datawidth:

## Macros
#define | LL_QSPI_DATASIZE_4BIT (3UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 4 bits. More...
#define | LL_QSPI_DATASIZE_5BIT (4UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 5 bits. More...
#define | LL_QSPI_DATASIZE_6BIT (5UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 6 bits. More...
#define | LL_QSPI_DATASIZE_7BIT (6UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 7 bits. More...
#define | LL_QSPI_DATASIZE_8BIT (7UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 8 bits. More...
#define | LL_QSPI_DATASIZE_9BIT (8UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 9 bits. More...
#define | LL_QSPI_DATASIZE_10BIT (9UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 10 bits. More...
#define | LL_QSPI_DATASIZE_11BIT (10UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 11 bits. More...
#define | LL_QSPI_DATASIZE_12BIT (11UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 12 bits. More...
#define | LL_QSPI_DATASIZE_13BIT (12UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 13 bits. More...
#define | LL_QSPI_DATASIZE_14BIT (13UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 14 bits. More...
#define | LL_QSPI_DATASIZE_15BIT (14UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 15 bits. More...
#define | LL_QSPI_DATASIZE_16BIT (15UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 16 bits. More...
#define | LL_QSPI_DATASIZE_17BIT (16UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 17 bits. More...
#define | LL_QSPI_DATASIZE_18BIT (17UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 18 bits. More...
#define | LL_QSPI_DATASIZE_19BIT (18UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 19 bits. More...
#define | LL_QSPI_DATASIZE_20BIT (19UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 20 bits. More...
#define | LL_QSPI_DATASIZE_21BIT (20UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 21 bits. More...
#define | LL_QSPI_DATASIZE_22BIT (21UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 22 bits. More...
#define | LL_QSPI_DATASIZE_23BIT (22UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 23 bits. More...
#define | LL_QSPI_DATASIZE_24BIT (23UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 24 bits. More...
#define | LL_QSPI_DATASIZE_25BIT (24UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 25 bits. More...
#define | LL_QSPI_DATASIZE_26BIT (25UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 26 bits. More...
#define | LL_QSPI_DATASIZE_27BIT (26UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 27 bits. More...
#define | LL_QSPI_DATASIZE_28BIT (27UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 28 bits. More...
#define | LL_QSPI_DATASIZE_29BIT (28UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 29 bits. More...
#define | LL_QSPI_DATASIZE_30BIT (29UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 30 bits. More...
#define | LL_QSPI_DATASIZE_31BIT (30UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 31 bits. More...
#define | LL_QSPI_DATASIZE_32BIT (31UL << QSPI_CTRL0_DFS32_Pos)
| Data length for SPI transfer: 32 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_DATASIZE_10BIT

#define LL_QSPI_DATASIZE_10BIT (9UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 10 bits.

Definition at line 394 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_11BIT

#define LL_QSPI_DATASIZE_11BIT (10UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 11 bits.

Definition at line 395 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_12BIT

#define LL_QSPI_DATASIZE_12BIT (11UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 12 bits.

Definition at line 396 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_13BIT

#define LL_QSPI_DATASIZE_13BIT (12UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 13 bits.

Definition at line 397 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_14BIT

#define LL_QSPI_DATASIZE_14BIT (13UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 14 bits.

Definition at line 398 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_15BIT

#define LL_QSPI_DATASIZE_15BIT (14UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 15 bits.

Definition at line 399 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_16BIT

#define LL_QSPI_DATASIZE_16BIT (15UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 16 bits.

Definition at line 400 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_17BIT

#define LL_QSPI_DATASIZE_17BIT (16UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 17 bits.

Definition at line 401 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_18BIT

#define LL_QSPI_DATASIZE_18BIT (17UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 18 bits.

Definition at line 402 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_19BIT

#define LL_QSPI_DATASIZE_19BIT (18UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 19 bits.

Definition at line 403 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_20BIT

#define LL_QSPI_DATASIZE_20BIT (19UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 20 bits.

Definition at line 404 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_21BIT

#define LL_QSPI_DATASIZE_21BIT (20UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 21 bits.

Definition at line 405 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_22BIT

#define LL_QSPI_DATASIZE_22BIT (21UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 22 bits.

Definition at line 406 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_23BIT

#define LL_QSPI_DATASIZE_23BIT (22UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 23 bits.

Definition at line 407 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_24BIT

#define LL_QSPI_DATASIZE_24BIT (23UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 24 bits.

Definition at line 408 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_25BIT

#define LL_QSPI_DATASIZE_25BIT (24UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 25 bits.

Definition at line 409 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_26BIT

#define LL_QSPI_DATASIZE_26BIT (25UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 26 bits.

Definition at line 410 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_27BIT

#define LL_QSPI_DATASIZE_27BIT (26UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 27 bits.

Definition at line 411 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_28BIT

#define LL_QSPI_DATASIZE_28BIT (27UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 28 bits.

Definition at line 412 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_29BIT

#define LL_QSPI_DATASIZE_29BIT (28UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 29 bits.

Definition at line 413 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_30BIT

#define LL_QSPI_DATASIZE_30BIT (29UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 30 bits.

Definition at line 414 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_31BIT

#define LL_QSPI_DATASIZE_31BIT (30UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 31 bits.

Definition at line 415 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_32BIT

#define LL_QSPI_DATASIZE_32BIT (31UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 32 bits.

Definition at line 416 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_4BIT

#define LL_QSPI_DATASIZE_4BIT (3UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 4 bits.

Definition at line 388 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_5BIT

#define LL_QSPI_DATASIZE_5BIT (4UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 5 bits.

Definition at line 389 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_6BIT

#define LL_QSPI_DATASIZE_6BIT (5UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 6 bits.

Definition at line 390 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_7BIT

#define LL_QSPI_DATASIZE_7BIT (6UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 7 bits.

Definition at line 391 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_8BIT

#define LL_QSPI_DATASIZE_8BIT (7UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 8 bits.

Definition at line 392 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DATASIZE_9BIT

#define LL_QSPI_DATASIZE_9BIT (8UL << QSPI_CTRL0_DFS32_Pos)

Data length for SPI transfer: 9 bits.

Definition at line 393 of file gr55xx_ll_qspi.h.