Public Attributes | List of all members
dma_scatter_config Struct Reference
Peripheral Driver » HAL Driver » DMA » Structures » DMA Configuration

LL DMA scatter config definition. More...

`#include <gr55xx_hal_dma.h>`

## Public Attributes
uint32_t | dst_scatter_en
| Specifies the destination scatter function enable. More...
uint32_t | dst_dsi
| Specifies the destination scatter tnterval. More...
uint32_t | dst_dsc
| Specifies the destination scatter count. More...

## Detailed Description

LL DMA scatter config definition.

Definition at line 164 of file gr55xx_hal_dma.h.

## Member Data Documentation

## ◆ dst_dsc

uint32_t dma_scatter_config::dst_dsc

Specifies the destination scatter count.

This parameter can be a value between Min_Data = 0 and Max_Data = 0xFFF.

Definition at line 173 of file gr55xx_hal_dma.h.

## ◆ dst_dsi

uint32_t dma_scatter_config::dst_dsi

Specifies the destination scatter tnterval.

This parameter can be a value between Min_Data = 0 and Max_Data = 0xFFFFF.

Definition at line 170 of file gr55xx_hal_dma.h.

## ◆ dst_scatter_en

uint32_t dma_scatter_config::dst_scatter_en

Specifies the destination scatter function enable.

This parameter can be a value of Destination Scatter Enable.

Definition at line 167 of file gr55xx_hal_dma.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_dma.h