Macros
DMA Defines
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for DMA Defines:

## Macros
#define | LL_QSPI_DMA_TX_DIS 0x00000000UL
| Disable the transmit FIFO DMA channel. More...
#define | LL_QSPI_DMA_TX_EN QSPI_DMAC_TDMAE
| Enable the transmit FIFO DMA channel More...
#define | LL_QSPI_DMA_RX_DIS 0x00000000UL
| Disable the receive FIFO DMA channel. More...
#define | LL_QSPI_DMA_RX_EN QSPI_DMAC_RDMAE
| Enable the receive FIFO DMA channel More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_DMA_RX_DIS

#define LL_QSPI_DMA_RX_DIS 0x00000000UL

Disable the receive FIFO DMA channel.

Definition at line 511 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DMA_RX_EN

#define LL_QSPI_DMA_RX_EN QSPI_DMAC_RDMAE

Enable the receive FIFO DMA channel

Definition at line 512 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DMA_TX_DIS

#define LL_QSPI_DMA_TX_DIS 0x00000000UL

Disable the transmit FIFO DMA channel.

Definition at line 508 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_DMA_TX_EN

#define LL_QSPI_DMA_TX_EN QSPI_DMAC_TDMAE

Enable the transmit FIFO DMA channel

Definition at line 509 of file gr55xx_ll_qspi.h.