Enumerations
Enumerations
SYSTEM » Power Manager
Collaboration diagram for Enumerations:

## Enumerations
enum | boot_mode_t { COLD_BOOT = 0, WARM_BOOT }
| power manager boot type. More...
enum | pwr_mgmt_mode_t { PMR_MGMT_ACTIVE_MODE = 0x0, PMR_MGMT_IDLE_MODE, PMR_MGMT_SLEEP_MODE }
| power manager model. More...
enum | pwr_mgmt_dev_state_t { DEVICE_BUSY = 0x0, DEVICE_IDLE }
| power manager device work state. More...
enum | notify_timer_event_t { EVENT_APP_TIMER_START = 0, EVENT_APP_TIMER_STOP }
| power manager app timer work state. More...
enum | { BLE_GATT_COMMON_EVT_MTU_EXCHANGE = BLE_GATT_COMMON_EVT_BASE, BLE_GATT_COMMON_EVT_PRF_REGISTER, BLE_GATT_COMMON_EVT_MAX, ISO_GPIO_MASK_0 = 0x1, ISO_GPIO_MASK_1 = 0x2, ISO_GPIO_MASK_2 = 0x4, ISO_GPIO_MASK_3 = 0x8, ISO_GPIO_MASK_4 = 0x10, ISO_GPIO_MASK_5 = 0x20, ISO_GPIO_MASK_6 = 0x40, ISO_GPIO_MASK_7 = 0x80, AMS_PLAYER_ATTR_ID_NAME, AMS_PLAYER_ATTR_ID_PLAYBACK_INFO, AMS_PLAYER_ATTR_ID_VOLUME, IAS_ALERT_NONE, IAS_ALERT_MILD, IAS_ALERT_HIGH, TRC_PWR_WFE_MODE = 0, TRC_PWR_DSLEEP_MODE, TRC_PWR_ACTIVE_MODE, TRC_PWR_BLE_RET_DSLEEP, TRC_PWR_APP_TIMER_REFUSE, TRC_PWR_APP_TIMER_PASS, TRC_PWR_BLE_TIMER_REFUSE, TRC_PWR_BLE_TIMER_PASS, TRC_PWR_RTC_TIMER_REFUSE, TRC_PWR_RTC_TIMER_PASS, TRC_PWR_RTC1_TIMER_REFUSE, TRC_PWR_RTC1_TIMER_PASS, TRC_PWR_WDT_TIMER_REFUSE, TRC_PWR_WDT_TIMER_PASS }
| PMU Tracking. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ anonymous enum

anonymous enum

PMU Tracking.

Enumerator
BLE_GATT_COMMON_EVT_MTU_EXCHANGE | MTU Exchange event.
BLE_GATT_COMMON_EVT_PRF_REGISTER | Service Register event.
BLE_GATT_COMMON_EVT_MAX |
ISO_GPIO_MASK_0 |
ISO_GPIO_MASK_1 |
ISO_GPIO_MASK_2 |
ISO_GPIO_MASK_3 |
ISO_GPIO_MASK_4 |
ISO_GPIO_MASK_5 |
ISO_GPIO_MASK_6 |
ISO_GPIO_MASK_7 |
AMS_PLAYER_ATTR_ID_NAME | Player attribute index of name.
AMS_PLAYER_ATTR_ID_PLAYBACK_INFO | Player attribute index of playback information.
AMS_PLAYER_ATTR_ID_VOLUME | Player attribute index of volume.
IAS_ALERT_NONE | No alert.
IAS_ALERT_MILD | Mild alert.
IAS_ALERT_HIGH | High alert.
TRC_PWR_WFE_MODE | WFE mode.
TRC_PWR_DSLEEP_MODE | Deep sleep mode.
TRC_PWR_ACTIVE_MODE | Active mode.
TRC_PWR_BLE_RET_DSLEEP | BLE return deep sleep.
TRC_PWR_APP_TIMER_REFUSE | App timer refuse.
TRC_PWR_APP_TIMER_PASS | App timer pass.
TRC_PWR_BLE_TIMER_REFUSE | BLE timer refuse.
TRC_PWR_BLE_TIMER_PASS | BLE timer pass.
TRC_PWR_RTC_TIMER_REFUSE | RTC timer refuse.
TRC_PWR_RTC_TIMER_PASS | RTC timer pass.
TRC_PWR_RTC1_TIMER_REFUSE | RTC timer refuse.
TRC_PWR_RTC1_TIMER_PASS | RTC timer pass.
TRC_PWR_WDT_TIMER_REFUSE | AON WDT timer refuse.
TRC_PWR_WDT_TIMER_PASS | AON WDT timer pass.

Definition at line 128 of file gr55xx_pwr.h.

## ◆ boot_mode_t

enum boot_mode_t

power manager boot type.

Enumerator
COLD_BOOT | Cold boot state.
WARM_BOOT | Warm boot state.

Definition at line 99 of file gr55xx_pwr.h.

## ◆ notify_timer_event_t

enum notify_timer_event_t

power manager app timer work state.

Enumerator
EVENT_APP_TIMER_START | App-timer start state.
EVENT_APP_TIMER_STOP | App-timer stop state.

Definition at line 121 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_dev_state_t

enum pwr_mgmt_dev_state_t

power manager device work state.

Enumerator
DEVICE_BUSY | Device busy state.
DEVICE_IDLE | Device idle state.

Definition at line 114 of file gr55xx_pwr.h.

## ◆ pwr_mgmt_mode_t

enum pwr_mgmt_mode_t

power manager model.

Enumerator
PMR_MGMT_ACTIVE_MODE | Full speed state.
PMR_MGMT_IDLE_MODE | Idle state.
PMR_MGMT_SLEEP_MODE | Deep sleep state.

Definition at line 106 of file gr55xx_pwr.h.