Macros
UART Interrupt_definition
Peripheral Driver » HAL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for UART Interrupt_definition:

## Macros
#define | UART_IT_MS LL_UART_IER_MS
| Enable Modem Status Interrupt. More...
#define | UART_IT_RLS LL_UART_IER_RLS
| Enable Receiver Line Status Interrupt. More...
#define | UART_IT_THRE LL_UART_IER_THRE
| Enable Transmit Holding Register Empty Interrupt. More...
#define | UART_IT_RDA LL_UART_IER_RDA
| Enable Received Data Available Interrupt and Character Timeout Interrupt. More...

## Detailed Description

## Macro Definition Documentation

## ◆ UART_IT_MS

#define UART_IT_MS LL_UART_IER_MS

Enable Modem Status Interrupt.

Definition at line 296 of file gr55xx_hal_uart.h.

## ◆ UART_IT_RDA

#define UART_IT_RDA LL_UART_IER_RDA

Enable Received Data Available Interrupt and Character Timeout Interrupt.

Definition at line 299 of file gr55xx_hal_uart.h.

## ◆ UART_IT_RLS

#define UART_IT_RLS LL_UART_IER_RLS

Enable Receiver Line Status Interrupt.

Definition at line 297 of file gr55xx_hal_uart.h.

## ◆ UART_IT_THRE

#define UART_IT_THRE LL_UART_IER_THRE

Enable Transmit Holding Register Empty Interrupt.

Definition at line 298 of file gr55xx_hal_uart.h.