Public Attributes | List of all members
hts_meas_val_t Struct Reference
BLE Services » Health Thermometer Service (HTS) » Structures

Health Theromometer Measurement Character value structure. More...

`#include <hts.h>`

Collaboration diagram for hts_meas_val_t:
[legend]

## Public Attributes
hts_temp_meas_type_t | temp_meas_type
| Stable or intermediary type of temperature. More...
uint16_t | temp_original_value
| Temperature measurement original value. More...
ieee_float32_t | temp_convert_value
| Temperature measurement convert value. More...
hts_date_time_t | time_stamp
| Time Stamp. More...
hts_temp_meas_loc_t | temp_type
| Temperature Type measurement location. More...

## Detailed Description

Health Theromometer Measurement Character value structure.

Definition at line 194 of file hts.h.

## Member Data Documentation

## ◆ temp_convert_value

ieee_float32_t hts_meas_val_t::temp_convert_value

Temperature measurement convert value.

Definition at line 198 of file hts.h.

## ◆ temp_meas_type

hts_temp_meas_type_t hts_meas_val_t::temp_meas_type

Stable or intermediary type of temperature.

Definition at line 196 of file hts.h.

## ◆ temp_original_value

uint16_t hts_meas_val_t::temp_original_value

Temperature measurement original value.

Definition at line 197 of file hts.h.

## ◆ temp_type

hts_temp_meas_loc_t hts_meas_val_t::temp_type

Temperature Type measurement location.

Definition at line 200 of file hts.h.

## ◆ time_stamp

hts_date_time_t hts_meas_val_t::time_stamp

Time Stamp.

Definition at line 199 of file hts.h.

The documentation for this struct was generated from the following file:

- hts.h