Public Attributes | List of all members
ascp_gap_cb_fun_t Struct Reference
BLE » Core Isochronous Channels » Structures

The callback for gap event which need to be handled by ascp. More...

`#include <ble_iso.h>`

## Public Attributes
void(* | gap_adv_report_ind_cb )(const ble_gap_ext_adv_report_ind_t *p_adv_report)
| The callback for receving adv report event. More...
void(* | gap_sync_established_cb )(uint8_t inst_idx, uint8_t status, const ble_gap_sync_established_ind_t *p_sync_est_evt)
| The callback for receving sync periodic adv success event. More...

## Detailed Description

The callback for gap event which need to be handled by ascp.

Definition at line 662 of file ble_iso.h.

## Member Data Documentation

## ◆ gap_adv_report_ind_cb

void(* ascp_gap_cb_fun_t::gap_adv_report_ind_cb) (const ble_gap_ext_adv_report_ind_t *p_adv_report)

The callback for receving adv report event.

Definition at line 664 of file ble_iso.h.

## ◆ gap_sync_established_cb

void(* ascp_gap_cb_fun_t::gap_sync_established_cb) (uint8_t inst_idx, uint8_t status, const ble_gap_sync_established_ind_t *p_sync_est_evt)

The callback for receving sync periodic adv success event.

Definition at line 666 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h