Public Attributes | List of all members
_aon_gpio_init Struct Reference
Peripheral Driver » HAL Driver » AON_GPIO » Structures

AON_GPIO init structure definition. More...

`#include <gr55xx_hal_aon_gpio.h>`

## Public Attributes
uint32_t | pin
| Specifies the AON_GPIO pins to be configured. More...
uint32_t | mode
| Specifies the operating mode for the selected pins. More...
uint32_t | pull
| Specifies the Pull-up or Pull-Down activation for the selected pins. More...
uint32_t | mux
| Specifies the Peripheral to be connected to the selected pins. More...

## Detailed Description

AON_GPIO init structure definition.

Definition at line 86 of file gr55xx_hal_aon_gpio.h.

## Member Data Documentation

## ◆ mode

uint32_t _aon_gpio_init::mode

Specifies the operating mode for the selected pins.

This parameter can be a value of AON_GPIO mode

Definition at line 91 of file gr55xx_hal_aon_gpio.h.

## ◆ mux

uint32_t _aon_gpio_init::mux

Specifies the Peripheral to be connected to the selected pins.

This parameter can be a value of GPIOEx Mux function selection.

Definition at line 97 of file gr55xx_hal_aon_gpio.h.

## ◆ pin

uint32_t _aon_gpio_init::pin

Specifies the AON_GPIO pins to be configured.

This parameter can be any value of AON_GPIO pins

Definition at line 88 of file gr55xx_hal_aon_gpio.h.

## ◆ pull

uint32_t _aon_gpio_init::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

This parameter can be a value of AON_GPIO pull

Definition at line 94 of file gr55xx_hal_aon_gpio.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_aon_gpio.h