Enumerations
Enumerations
BLE Services » Power Consumption Service (PCS)
Collaboration diagram for Enumerations:

## Enumerations
enum | pcs_evt_type_t { PCS_EVT_INVALID, PCS_EVT_TX_ENABLE, PCS_EVT_TX_DISABLE, PCS_EVT_SETTING_ENABLE, PCS_EVT_SETTING_DISABLE, PCS_EVT_TX_DATA_SENT, PCS_EVT_PARAM_SET, PCS_EVT_DISCONNECTED }
| PCS Service event types. More...
enum | pcs_setting_type_t { PCS_SETTING_TYPE_ADV_INTERVAL, PCS_SETTING_TYPE_CONN_PARAM, PCS_SETTING_TYPE_PHY, PCS_SETTING_TYPE_ADV_DATA, PCS_SETTING_TYPE_TX_POWER }
| PCS Service settings types. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ pcs_evt_type_t

enum pcs_evt_type_t

PCS Service event types.

Enumerator
PCS_EVT_INVALID | Invalid PCS event.
PCS_EVT_TX_ENABLE | TX notify has been enabled.
PCS_EVT_TX_DISABLE | TX notify has been disabled.
PCS_EVT_SETTING_ENABLE | Setting notify has been enabled.
PCS_EVT_SETTING_DISABLE | Setting notify has been disabled.
PCS_EVT_TX_DATA_SENT | Data has been notitied completely.
PCS_EVT_PARAM_SET | BLE parameters set.
PCS_EVT_DISCONNECTED | Disconnected.

Definition at line 88 of file pcs.h.

## ◆ pcs_setting_type_t

enum pcs_setting_type_t

PCS Service settings types.

Enumerator
PCS_SETTING_TYPE_ADV_INTERVAL | BLE Advertising Interval parameter.
PCS_SETTING_TYPE_CONN_PARAM | BLE Connection parameter.
PCS_SETTING_TYPE_PHY | Radio Phy mode, 1M, 2M, Encoded.
PCS_SETTING_TYPE_ADV_DATA | BLE advertising data.
PCS_SETTING_TYPE_TX_POWER | Tx Power.

Definition at line 101 of file pcs.h.