Public Attributes | List of all members
gdx_lcp_config_t Struct Reference
BLE » Light Communication Protocol (LCP) » Structures

LCP Parameter. More...

`#include <ble_lcp.h>`

## Public Attributes
uint8_t | mode
| Set protocol mode, see PROTOCOL_MODE. More...
int8_t | txpwr_dbm
| The value of the tx power(range: -20-7), uint: dBm. More...
uint8_t | ch_idx
| The value of the channel index(range: 0-39). More...
uint32_t | freq
| The value of the frequency(range: 2360-2520), uint: MHz. More...
uint32_t | access_address
| The value of the access address. More...
uint32_t | crc_init
| The initial value of the crc. More...
rx_handler_cb_t | rx_handler_cb
| The callback function of rx. More...

## Detailed Description

LCP Parameter.

Definition at line 75 of file ble_lcp.h.

## Member Data Documentation

## ◆ access_address

uint32_t gdx_lcp_config_t::access_address

The value of the access address.

Definition at line 81 of file ble_lcp.h.

## ◆ ch_idx

uint8_t gdx_lcp_config_t::ch_idx

The value of the channel index(range: 0-39).

Definition at line 79 of file ble_lcp.h.

## ◆ crc_init

uint32_t gdx_lcp_config_t::crc_init

The initial value of the crc.

Definition at line 82 of file ble_lcp.h.

## ◆ freq

uint32_t gdx_lcp_config_t::freq

The value of the frequency(range: 2360-2520), uint: MHz.

Definition at line 80 of file ble_lcp.h.

## ◆ mode

uint8_t gdx_lcp_config_t::mode

Set protocol mode, see PROTOCOL_MODE.

Definition at line 77 of file ble_lcp.h.

## ◆ rx_handler_cb

rx_handler_cb_t gdx_lcp_config_t::rx_handler_cb

The callback function of rx.

Definition at line 83 of file ble_lcp.h.

## ◆ txpwr_dbm

int8_t gdx_lcp_config_t::txpwr_dbm

The value of the tx power(range: -20-7), uint: dBm.

Definition at line 78 of file ble_lcp.h.

The documentation for this struct was generated from the following file:

- ble_lcp.h