Enumerations
Enumerations
Graphics » HAL DC » GDC Intern
Collaboration diagram for Enumerations:

## Enumerations
enum | hal_gdc_colormode_check_t { HAL_GDC_DBIB_STALL_CHK = 1 << 31, HAL_GDC_OPENLDI_CHK = 1U << 30, HAL_GDC_JDIMIP_CHK = 1U << 29, HAL_GDC_ARGB4444_CHK = 1U << 22, HAL_GDC_RGBA4444_CHK = 1U << 21, HAL_GDC_GPI_CHK = 1U << 20, HAL_GDC_EXTRCTRL_CHK = 1U << 19, HAL_GDC_TSC6_CHK = 1U << 18, HAL_GDC_TSC_CHK = 1U << 17, HAL_GDC_LUT8_CHK = 1U << 16, HAL_GDC_RGBA5551_CHK = 1U << 15, HAL_GDC_ABGR8888_CHK = 1U << 14, HAL_GDC_RGB332_CHK = 1U << 13, HAL_GDC_RGB565_CHK = 1U << 12, HAL_GDC_BGRA8888_CHK = 1U << 11, HAL_GDC_L8_CHK = 1U << 10, HAL_GDC_L1_CHK = 1U << 9, HAL_GDC_L4_CHK = 1U << 8, HAL_GDC_YUVV_CHK = 1U << 7, HAL_GDC_RGB24_CHK = 1U << 6, HAL_GDC_YUY2_CHK = 1U << 5, HAL_GDC_RGBA8888_CHK = 1U << 4, HAL_GDC_ARGB8888_CHK = 1U << 3, HAL_GDC_V_YUV420_CHK = 1U << 2, HAL_GDC_TLYUV420_CHK = 1U << 1, HAL_GDC_BLOCK4X4_CHK = 1U << 0 }
| DC's color mode check definition. More...
enum | hal_gdc_AXI_cfg_t { HAL_GDC_AXI_16BEAT = 0x0, HAL_GDC_AXI_2BEAT = 0x1, HAL_GDC_AXI_4BEAT = 0x2, HAL_GDC_AXI_8BEAT = 0x3, HAL_GDC_AXI_32BEAT = 0x5, HAL_GDC_AXI_64BEAT = 0x6, HAL_GDC_AXI_128BEAT = 0x7, HAL_GDC_AXI_FT_HF = 0x0U << 3, HAL_GDC_AXI_FT_2B = 0x1U << 3, HAL_GDC_AXI_FT_4B = 0x2U << 3, HAL_GDC_AXI_FT_8B = 0x3U << 3 }
| AXI control definition. More...
enum | dc_mipi_cmd_t { hal_gdc_snapshot = 0xff, hal_gdc_store_base_addr = (1 <<31), hal_gdc_DBI_cmd = (1U<<30), hal_gdc_wcmd16 = (1U<<28), hal_gdc_wcmd24 = (1U<<29), hal_gdc_wcmd32 = (1U<<29)|(1U<<28), hal_gdc_rcmd16 = (1U<<28), hal_gdc_rcmd24 = (1U<<29), hal_gdc_rcmd32 = (1U<<29)|(1U<<28), hal_gdc_mask_qspi = (1U<<27), hal_gdc_DBI_ge = (1U<<27), hal_gdc_DBI_read = (1U<<26), hal_gdc_ext_ctrl = (1U<<25), hal_gdc_sline_cmd = (1U<<24), hal_gdc_read_byte = (0U<<30), hal_gdc_read_2byte = (1U<<30), hal_gdc_read_3byte = (2 <<30), hal_gdc_read_4byte = (3 <<30) }
| MIPI CMD definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ dc_mipi_cmd_t

enum dc_mipi_cmd_t

MIPI CMD definition.

Enumerator
hal_gdc_snapshot | Snapshot.
hal_gdc_store_base_addr | Store base addr.
hal_gdc_DBI_cmd | DBI CMD.
hal_gdc_wcmd16 | Write CMD 16bits.
hal_gdc_wcmd24 | Write CMD 24bits.
hal_gdc_wcmd32 | Write CMD 32bits.
hal_gdc_rcmd16 | Read CMD 16bits.
hal_gdc_rcmd24 | Read CMD 24its.
hal_gdc_rcmd32 | Read CMD 32bits.
hal_gdc_mask_qspi | Force QSPI to be single wire.
hal_gdc_DBI_ge | DBI ge.
hal_gdc_DBI_read | DBI read.
hal_gdc_ext_ctrl | Ext control.
hal_gdc_sline_cmd | Sline CMD.
hal_gdc_read_byte | Read 1Byte.
hal_gdc_read_2byte | Read 2Byte.
hal_gdc_read_3byte | Read 3Byte.
hal_gdc_read_4byte | Read 4Byte.

Definition at line 132 of file hal_gdc_intern.h.

## ◆ hal_gdc_AXI_cfg_t

enum hal_gdc_AXI_cfg_t

AXI control definition.

Enumerator
HAL_GDC_AXI_16BEAT | 16 beat
HAL_GDC_AXI_2BEAT | 2beat
HAL_GDC_AXI_4BEAT | 4 beat
HAL_GDC_AXI_8BEAT | 8 beat
HAL_GDC_AXI_32BEAT | 32 beat
HAL_GDC_AXI_64BEAT | 64 beat
HAL_GDC_AXI_128BEAT | 128 beat
HAL_GDC_AXI_FT_HF | Ignore.
HAL_GDC_AXI_FT_2B | Ignore.
HAL_GDC_AXI_FT_4B | Ignore.
HAL_GDC_AXI_FT_8B | Ignore.

Definition at line 115 of file hal_gdc_intern.h.

## ◆ hal_gdc_colormode_check_t

enum hal_gdc_colormode_check_t

DC's color mode check definition.

Enumerator
HAL_GDC_DBIB_STALL_CHK | DBIB stall check.
HAL_GDC_OPENLDI_CHK | Openldi check.
HAL_GDC_JDIMIP_CHK | JDIMIP check.
HAL_GDC_ARGB4444_CHK | ARGB444 check.
HAL_GDC_RGBA4444_CHK | RGBA444 check.
HAL_GDC_GPI_CHK | GPI check.
HAL_GDC_EXTRCTRL_CHK | EXTRCTRL check.
HAL_GDC_TSC6_CHK | TSC6 check.
HAL_GDC_TSC_CHK | TSC check.
HAL_GDC_LUT8_CHK | LUT8 check.
HAL_GDC_RGBA5551_CHK | RGBA5551 check.
HAL_GDC_ABGR8888_CHK | ARGB8888 check.
HAL_GDC_RGB332_CHK | RGB332 check.
HAL_GDC_RGB565_CHK | RGB565 check.
HAL_GDC_BGRA8888_CHK | BGRA8888 check.
HAL_GDC_L8_CHK | L8 check.
HAL_GDC_L1_CHK | L1 check.
HAL_GDC_L4_CHK | L4 check.
HAL_GDC_YUVV_CHK | YUVV check.
HAL_GDC_RGB24_CHK | RGB24 check.
HAL_GDC_YUY2_CHK | YUV2 check.
HAL_GDC_RGBA8888_CHK | RGBA8888 check.
HAL_GDC_ARGB8888_CHK | ARGB8888 check.
HAL_GDC_V_YUV420_CHK | V_YUV420 check.
HAL_GDC_TLYUV420_CHK | TLYUV420 check.
HAL_GDC_BLOCK4X4_CHK | BLOCK4X4 check.

Definition at line 83 of file hal_gdc_intern.h.