Macros
endian mode for qspi xip
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for endian mode for qspi xip:

## Macros
#define | QSPI_CONCURRENT_XIP_ENDIAN_MODE_0 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0
| Default endian order from AHB. More...
#define | QSPI_CONCURRENT_XIP_ENDIAN_MODE_1 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1
| Re-order the read data as [23:16], [31:24], [7:0], [15:8]. More...
#define | QSPI_CONCURRENT_XIP_ENDIAN_MODE_2 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2
| Re-order the read data as [7:0], [15:8], [23:16], [31:24]. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_ENDIAN_MODE_0

#define QSPI_CONCURRENT_XIP_ENDIAN_MODE_0 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_0

Default endian order from AHB.

Definition at line 569 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ENDIAN_MODE_1

#define QSPI_CONCURRENT_XIP_ENDIAN_MODE_1 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_1

Re-order the read data as [23:16], [31:24], [7:0], [15:8].

Definition at line 570 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ENDIAN_MODE_2

#define QSPI_CONCURRENT_XIP_ENDIAN_MODE_2 LL_QSPI_CONCURRENT_XIP_ENDIAN_MODE_2

Re-order the read data as [7:0], [15:8], [23:16], [31:24].

Definition at line 571 of file gr55xx_hal_qspi.h.