Macros
USB EF FIFO address
Peripheral Driver » HAL Driver » USB » Defines » USB Exported Constants
Collaboration diagram for USB EF FIFO address:

## Macros
#define | HAL_USB_FIFO_EP0 (USB_BASE + 0x40)
| USB EP0 FIFO address. More...
#define | HAL_USB_FIFO_EP1 (USB_BASE + 0x44)
| USB EP1 FIFO address. More...
#define | HAL_USB_FIFO_EP2 (USB_BASE + 0x48)
| USB EP2 FIFO address. More...
#define | HAL_USB_FIFO_EP3 (USB_BASE + 0x4C)
| USB EP3 FIFO address. More...

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_USB_FIFO_EP0

#define HAL_USB_FIFO_EP0 (USB_BASE + 0x40)

USB EP0 FIFO address.

Definition at line 278 of file gr55xx_hal_usb.h.

## ◆ HAL_USB_FIFO_EP1

#define HAL_USB_FIFO_EP1 (USB_BASE + 0x44)

USB EP1 FIFO address.

Definition at line 279 of file gr55xx_hal_usb.h.

## ◆ HAL_USB_FIFO_EP2

#define HAL_USB_FIFO_EP2 (USB_BASE + 0x48)

USB EP2 FIFO address.

Definition at line 280 of file gr55xx_hal_usb.h.

## ◆ HAL_USB_FIFO_EP3

#define HAL_USB_FIFO_EP3 (USB_BASE + 0x4C)

USB EP3 FIFO address.

Definition at line 281 of file gr55xx_hal_usb.h.