Public Attributes | List of all members
_qspi_init_t Struct Reference
Peripheral Driver » HAL Driver » QSPI » Structures » QSPI Configuration

QSPI init Structure definition. More...

`#include <gr55xx_hal_qspi.h>`

## Public Attributes
uint32_t | clock_prescaler
| Specifies the prescaler factor for generating clock based on the AHB clock. More...
uint32_t | clock_mode
| Specifies the Clock Mode. More...
uint32_t | rx_sample_delay
| Specifies the RX sample delay. More...

## Detailed Description

QSPI init Structure definition.

Definition at line 136 of file gr55xx_hal_qspi.h.

## Member Data Documentation

## ◆ clock_mode

uint32_t _qspi_init_t::clock_mode

Specifies the Clock Mode.

It indicates the level that clock takes between commands. This parameter can be a value of QSPI Clock Mode.

Definition at line 141 of file gr55xx_hal_qspi.h.

## ◆ clock_prescaler

uint32_t _qspi_init_t::clock_prescaler

Specifies the prescaler factor for generating clock based on the AHB clock.

This parameter can be a number between 0 and 0xFFFF.

Definition at line 138 of file gr55xx_hal_qspi.h.

## ◆ rx_sample_delay

uint32_t _qspi_init_t::rx_sample_delay

Specifies the RX sample delay.

It is used to delay the sample of the RX input port. This parameter can be a number between 0 and 0x7.

Definition at line 144 of file gr55xx_hal_qspi.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_qspi.h