Modules | Macros
Defines
BLE Services » Health Thermometer Service (HTS)
Collaboration diagram for Defines:

## Modules
| Characteristics Mask
| Bit masks for the initialization of hts_init_t::char_mask.

## Macros
#define | HTS_CONNECTION_MAX 10
| Maximum number of Health Thermometer Service connections. More...
#define | HTS_TEM_MEAS_MAX_LEN 20
| Maximum length of temperature measurement encode. More...
#define | HTS_TEM_TYPE_MAX_LEN 1
| Maximum length of temperature type value. More...
#define | HTS_INTM_TEM_MAX_LEN 20
| Maximun length of intermediate temperature encode. More...
#define | HTS_MEAS_INTERVAL_MAX_LEN 2
| Maximum length of measurement interval value. More...
#define | HTS_MEAS_INTV_DFLT_MIN 2
| Minimun interval of temperature measurement (in unit of 1s). More...
#define | HTS_MEAS_INTV_DFLT_MAX 10
| Maximum interval of temperature measurement (in unit of 1s). More...

## Detailed Description

## Macro Definition Documentation

## ◆ HTS_CONNECTION_MAX

#define HTS_CONNECTION_MAX 10

Maximum number of Health Thermometer Service connections.

Definition at line 74 of file hts.h.

## ◆ HTS_INTM_TEM_MAX_LEN

#define HTS_INTM_TEM_MAX_LEN 20

Maximun length of intermediate temperature encode.

Definition at line 77 of file hts.h.

## ◆ HTS_MEAS_INTERVAL_MAX_LEN

#define HTS_MEAS_INTERVAL_MAX_LEN 2

Maximum length of measurement interval value.

Definition at line 78 of file hts.h.

## ◆ HTS_MEAS_INTV_DFLT_MAX

#define HTS_MEAS_INTV_DFLT_MAX 10

Maximum interval of temperature measurement (in unit of 1s).

Definition at line 80 of file hts.h.

## ◆ HTS_MEAS_INTV_DFLT_MIN

#define HTS_MEAS_INTV_DFLT_MIN 2

Minimun interval of temperature measurement (in unit of 1s).

Definition at line 79 of file hts.h.

## ◆ HTS_TEM_MEAS_MAX_LEN

#define HTS_TEM_MEAS_MAX_LEN 20

Maximum length of temperature measurement encode.

Definition at line 75 of file hts.h.

## ◆ HTS_TEM_TYPE_MAX_LEN

#define HTS_TEM_TYPE_MAX_LEN 1

Maximum length of temperature type value.

Definition at line 76 of file hts.h.