Macros
Characteristics Mask
BLE Services » Heart Rate Service (HRS) » Defines

Bit masks for the initialization of hrs_init_t::char_mask. More...

Collaboration diagram for Characteristics Mask:

## Macros
#define | HRS_CHAR_MANDATORY 0x0F
| Bit mask of the mandatory characteristics. More...
#define | HRS_CHAR_BODY_SENSOR_LOC_SUP 0x30
| Bit mask of Body Sensor Location Feature Supported. More...
#define | HRS_CHAR_ENGY_EXP_SUP 0xC0
| Bit mask of Energy Expanded Feature Supported. More...

## Detailed Description

Bit masks for the initialization of hrs_init_t::char_mask.

## Macro Definition Documentation

## ◆ HRS_CHAR_BODY_SENSOR_LOC_SUP

#define HRS_CHAR_BODY_SENSOR_LOC_SUP 0x30

Bit mask of Body Sensor Location Feature Supported.

Definition at line 92 of file hrs.h.

## ◆ HRS_CHAR_ENGY_EXP_SUP

#define HRS_CHAR_ENGY_EXP_SUP 0xC0

Bit mask of Energy Expanded Feature Supported.

Definition at line 93 of file hrs.h.

## ◆ HRS_CHAR_MANDATORY

#define HRS_CHAR_MANDATORY 0x0F

Bit mask of the mandatory characteristics.

Definition at line 91 of file hrs.h.