Macros
Data Frame Size For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

Data frame size in xip, take effect when enable DFS_HC. More...

Collaboration diagram for Data Frame Size For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_DATASIZE_8BIT
#define | LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_DATASIZE_16BIT
#define | LL_QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_DATASIZE_32BIT

## Detailed Description

Data frame size in xip, take effect when enable DFS_HC.

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_BYTE

#define LL_QSPI_CONCURRENT_XIP_DFS_BYTE LL_QSPI_DATASIZE_8BIT

Definition at line 581 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD

#define LL_QSPI_CONCURRENT_XIP_DFS_HALFWORD LL_QSPI_DATASIZE_16BIT

Definition at line 582 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_DFS_WORD

#define LL_QSPI_CONCURRENT_XIP_DFS_WORD LL_QSPI_DATASIZE_32BIT

Definition at line 583 of file gr55xx_ll_qspi.h.