Functions
MSIO_A_IRQHandler and Callbacks
Peripheral Driver » HAL Driver » MSIO » Functions

IRQ Handler and Callbacks functions. More...

Collaboration diagram for MSIO_A_IRQHandler and Callbacks:

## Functions
void | hal_msio_exti_irq_handler (msio_pad_t MSIOx)
| Handle MSIOA interrupt request. More...
void | hal_msio_exti_callback (msio_pad_t MSIOx, uint16_t msio_pin)
| MSIOA pin detection callback. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_msio_exti_callback()

void hal_msio_exti_callback | ( | msio_pad_t | MSIOx,
|  | uint16_t | msio_pin
| ) |  |

MSIOA pin detection callback.

Note
  This function should not be modified. When the callback is needed, the hal_msio_exti_callback can be implemented in the user file.

Parameters

  [in] | MSIOx | Must select the MSIOA port.
  [in] | msio_pin | Indicate the port pin whose interrupt was triggered. This parameter can be a combination of the following values: MSIO_PIN_0 MSIO_PIN_1 MSIO_PIN_2 MSIO_PIN_3 MSIO_PIN_4 MSIO_PIN_5 MSIO_PIN_6 MSIO_PIN_7 MSIO_PIN_ALL

## ◆ hal_msio_exti_irq_handler()

void hal_msio_exti_irq_handler | ( | msio_pad_t | MSIOx | ) |

Handle MSIOA interrupt request.

Parameters

  [in] | MSIOx | Must select the MSIOA port.