Macros
QSPI interrupt Defines
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants

Interrupt defines which can be used with LL_XQSPI_ReadReg and LL_XQSPI_WriteReg functions. More...

Collaboration diagram for QSPI interrupt Defines:

## Macros
#define | LL_XQSPI_QSPI_IM_DONE XQSPI_QSPI_XFER_DPULSE_Msk
| Transmite Done Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_RFF XQSPI_QSPI_RX_FPULSE_Msk
| Receive FIFO Full Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_RFTF XQSPI_QSPI_RX_WPULSE_Msk
| Receive FIFO Watermark Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_TFTF XQSPI_QSPI_TX_WPULSE_Msk
| Transmit FIFO Watermark Interrupt enable More...
#define | LL_XQSPI_QSPI_IM_TFE XQSPI_QSPI_TX_EPULSE_Msk
| Transmit FIFO Empty Interrupt enable More...
#define | LL_XQSPI_QSPI_IS_DONE XQSPI_QSPI_XFER_DPULSE_Msk
| Transmite Done Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_RFF XQSPI_QSPI_RX_FPULSE_Msk
| Receive FIFO Full Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_RFTF XQSPI_QSPI_RX_WPULSE_Msk
| Receive FIFO Watermark Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_TFTF XQSPI_QSPI_TX_WPULSE_Msk
| Transmit FIFO Watermark Interrupt flag More...
#define | LL_XQSPI_QSPI_IS_TFE XQSPI_QSPI_TX_EPULSE_Msk
| Transmit FIFO Empty Interrupt flag More...

## Detailed Description

Interrupt defines which can be used with LL_XQSPI_ReadReg and LL_XQSPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_XQSPI_QSPI_IM_DONE

#define LL_XQSPI_QSPI_IM_DONE XQSPI_QSPI_XFER_DPULSE_Msk

Transmite Done Interrupt enable

Definition at line 248 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_RFF

#define LL_XQSPI_QSPI_IM_RFF XQSPI_QSPI_RX_FPULSE_Msk

Receive FIFO Full Interrupt enable

Definition at line 249 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_RFTF

#define LL_XQSPI_QSPI_IM_RFTF XQSPI_QSPI_RX_WPULSE_Msk

Receive FIFO Watermark Interrupt enable

Definition at line 250 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_TFE

#define LL_XQSPI_QSPI_IM_TFE XQSPI_QSPI_TX_EPULSE_Msk

Transmit FIFO Empty Interrupt enable

Definition at line 252 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IM_TFTF

#define LL_XQSPI_QSPI_IM_TFTF XQSPI_QSPI_TX_WPULSE_Msk

Transmit FIFO Watermark Interrupt enable

Definition at line 251 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_DONE

#define LL_XQSPI_QSPI_IS_DONE XQSPI_QSPI_XFER_DPULSE_Msk

Transmite Done Interrupt flag

Definition at line 254 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_RFF

#define LL_XQSPI_QSPI_IS_RFF XQSPI_QSPI_RX_FPULSE_Msk

Receive FIFO Full Interrupt flag

Definition at line 255 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_RFTF

#define LL_XQSPI_QSPI_IS_RFTF XQSPI_QSPI_RX_WPULSE_Msk

Receive FIFO Watermark Interrupt flag

Definition at line 256 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_TFE

#define LL_XQSPI_QSPI_IS_TFE XQSPI_QSPI_TX_EPULSE_Msk

Transmit FIFO Empty Interrupt flag

Definition at line 258 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_IS_TFTF

#define LL_XQSPI_QSPI_IS_TFTF XQSPI_QSPI_TX_WPULSE_Msk

Transmit FIFO Watermark Interrupt flag

Definition at line 257 of file gr55xx_ll_xqspi.h.