### - g -

- GDC_IRQ_EVT_CMD_TRANSMITION_END : app_graphics_dc.h
- GDC_IRQ_EVT_FRAME_TRANSMITION_END : app_graphics_dc.h
- GGPU_IRQ_EVT_CMD_LIST_END : app_graphics_gpu.h
- GGPU_IRQ_EVT_DRAW_CMD_END : app_graphics_gpu.h
- GGPU_IRQ_EVT_IRQ_ID_CLEAR : app_graphics_gpu.h
- GGPU_IRQ_EVT_OTHER : app_graphics_gpu.h
- GLOBAL_EXCEPTION_DISABLE : gr55xx_hal.h
- GLOBAL_EXCEPTION_ENABLE : gr55xx_hal.h
- GLOBAL_INT_DISABLE : gr55xx_hal.h
- GLOBAL_INT_RESTORE : gr55xx_hal.h
- GPIO_ALTFUNCCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_ALTFUNCSET_ADDR : gr55xx_ll_gpio.h
- GPIO_DATA_ADDR : gr55xx_ll_gpio.h
- GPIO_DATAOUT_ADDR : gr55xx_ll_gpio.h
- GPIO_DEFAULT_CONFIG : gr55xx_hal_gpio.h
- GPIO_INTDBECLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTDBESET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTENCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTENSET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTPOLCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTPOLSET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTSTAT_ADDR : gr55xx_ll_gpio.h
- GPIO_INTTYPECLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTTYPESET_ADDR : gr55xx_ll_gpio.h
- GPIO_MODE_INPUT : gr55xx_hal_gpio.h
- GPIO_MODE_IT_BOTH_EDGE : gr55xx_hal_gpio.h
- GPIO_MODE_IT_FALLING : gr55xx_hal_gpio.h
- GPIO_MODE_IT_HIGH : gr55xx_hal_gpio.h
- GPIO_MODE_IT_LOW : gr55xx_hal_gpio.h
- GPIO_MODE_IT_RISING : gr55xx_hal_gpio.h
- GPIO_MODE_MUX : gr55xx_hal_gpio.h
- GPIO_MODE_OUTPUT : gr55xx_hal_gpio.h
- GPIO_MUX_0 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_1 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_2 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_3 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_4 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_5 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_6 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_7 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_8 : gr55xx_hal_gpio_ex.h
- GPIO_NOPULL : gr55xx_hal_gpio.h
- GPIO_OUTENCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_OUTENSET_ADDR : gr55xx_ll_gpio.h
- GPIO_PIN_0 : gr55xx_hal_gpio.h
- GPIO_PIN_1 : gr55xx_hal_gpio.h
- GPIO_PIN_10 : gr55xx_hal_gpio.h
- GPIO_PIN_11 : gr55xx_hal_gpio.h
- GPIO_PIN_12 : gr55xx_hal_gpio.h
- GPIO_PIN_13 : gr55xx_hal_gpio.h
- GPIO_PIN_14 : gr55xx_hal_gpio.h
- GPIO_PIN_15 : gr55xx_hal_gpio.h
- GPIO_PIN_2 : gr55xx_hal_gpio.h
- GPIO_PIN_3 : gr55xx_hal_gpio.h
- GPIO_PIN_4 : gr55xx_hal_gpio.h
- GPIO_PIN_5 : gr55xx_hal_gpio.h
- GPIO_PIN_6 : gr55xx_hal_gpio.h
- GPIO_PIN_7 : gr55xx_hal_gpio.h
- GPIO_PIN_8 : gr55xx_hal_gpio.h
- GPIO_PIN_9 : gr55xx_hal_gpio.h
- GPIO_PIN_ALL : gr55xx_hal_gpio.h
- GPIO_PIN_MASK : gr55xx_hal_gpio.h
- GPIO_PULLDOWN : gr55xx_hal_gpio.h
- GPIO_PULLUP : gr55xx_hal_gpio.h
- gr_assert_param : gr55xx_hal_conf.h
- GRAPHICS_DC_BASEADDR : app_graphics_dc.h
- GRAPHICS_DC_CLK_PIN : app_graphics_dc.h
- GRAPHICS_DC_CLK_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_CLK_PORT : app_graphics_dc.h
- GRAPHICS_DC_CSN_PIN : app_graphics_dc.h
- GRAPHICS_DC_CSN_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_CSN_PORT : app_graphics_dc.h
- GRAPHICS_DC_DCX_PIN : app_graphics_dc.h
- GRAPHICS_DC_DCX_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_DCX_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO0_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO0_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO0_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO1_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO1_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO1_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO2_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO2_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO2_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO3_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO3_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO3_PORT : app_graphics_dc.h
- GRAPHICS_DC_LAYER_0 : app_graphics_dc.h
- GRAPHICS_DC_LAYER_1 : app_graphics_dc.h
- GRAPHICS_GPU_BASEADDR : app_graphics_gpu.h
- GUS_C_CONNECTION_MAX : gus_c.h
- GUS_CONNECTION_MAX : gus.h
- GUS_FLOW_CTRL_LEN : gus.h
- GUS_FLOW_CTRL_UUID : gus_c.h
- GUS_MAX_DATA_LEN : gus.h
- GUS_RX_CHAR_UUID : gus_c.h
- GUS_SERVICE_UUID : gus.h
- GUS_SVC_UUID : gus_c.h
- GUS_TX_CHAR_UUID : gus_c.h