Macros
I2S Flags Definition
Peripheral Driver » HAL Driver » I2S » Defines » I2S Exported Constants
Collaboration diagram for I2S Flags Definition:

## Macros
#define | I2S_FLAG_TXFO LL_I2S_STATUS_TXFO
| TX FIFO write overflow flag More...
#define | I2S_FLAG_TXFE LL_I2S_STATUS_TXFE
| TX FIFO empty trigger flag More...
#define | I2S_FLAG_RXFO LL_I2S_STATUS_RXFO
| RX FIFO receive overflow flag More...
#define | I2S_FLAG_RXDA LL_I2S_STATUS_RXDA
| RX FIFO data available flag More...

## Detailed Description

## Macro Definition Documentation

## ◆ I2S_FLAG_RXDA

#define I2S_FLAG_RXDA LL_I2S_STATUS_RXDA

RX FIFO data available flag

Definition at line 267 of file gr55xx_hal_i2s.h.

## ◆ I2S_FLAG_RXFO

#define I2S_FLAG_RXFO LL_I2S_STATUS_RXFO

RX FIFO receive overflow flag

Definition at line 266 of file gr55xx_hal_i2s.h.

## ◆ I2S_FLAG_TXFE

#define I2S_FLAG_TXFE LL_I2S_STATUS_TXFE

TX FIFO empty trigger flag

Definition at line 265 of file gr55xx_hal_i2s.h.

## ◆ I2S_FLAG_TXFO

#define I2S_FLAG_TXFO LL_I2S_STATUS_TXFO

TX FIFO write overflow flag

Definition at line 264 of file gr55xx_hal_i2s.h.