Macros
Parity Control
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for Parity Control:

## Macros
#define | LL_UART_PARITY_NONE UART_LCR_PARITY_NONE
| Parity control disabled. More...
#define | LL_UART_PARITY_ODD UART_LCR_PARITY_ODD
| Parity control enabled and Odd Parity is selected. More...
#define | LL_UART_PARITY_EVEN UART_LCR_PARITY_EVEN
| Parity control enabled and Even Parity is selected. More...
#define | LL_UART_PARITY_SP0 UART_LCR_PARITY_SP0
| Parity control enabled and Stick Parity 0 is selected. More...
#define | LL_UART_PARITY_SP1 UART_LCR_PARITY_SP1
| Parity control enabled and Stick Parity 1 is selected. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_PARITY_EVEN

#define LL_UART_PARITY_EVEN UART_LCR_PARITY_EVEN

Parity control enabled and Even Parity is selected.

Definition at line 159 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_NONE

#define LL_UART_PARITY_NONE UART_LCR_PARITY_NONE

Parity control disabled.

Definition at line 157 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_ODD

#define LL_UART_PARITY_ODD UART_LCR_PARITY_ODD

Parity control enabled and Odd Parity is selected.

Definition at line 158 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_SP0

#define LL_UART_PARITY_SP0 UART_LCR_PARITY_SP0

Parity control enabled and Stick Parity 0 is selected.

Definition at line 160 of file gr55xx_ll_uart.h.

## ◆ LL_UART_PARITY_SP1

#define LL_UART_PARITY_SP1 UART_LCR_PARITY_SP1

Parity control enabled and Stick Parity 1 is selected.

Definition at line 161 of file gr55xx_ll_uart.h.