### - a -

- a : _color_var_t
- A : _ll_ecc_curve_init
- abort_reason : ras_subevt_data_t
- accept : ble_l2cap_enh_lecb_cfm_conn_t , ble_l2cap_lecb_cfm_conn_t , ble_sec_cfm_enc_t
- access_address : gdx_lcp_config_t
- ack_flag : ags_header_base_t , ags_stream_env_t
- ack_ra_data_param : ras_ctr_pt_operation_t
- acl_hdl : iso_req_peer_sca_cmpl_evt_t
- action_set : thscps_evt_t
- active_channel : app_pwm_params_t , pwm_handle_t
- adc_conv_cplt_callback : _hal_adc_callback
- adc_dma_state : adc_env_t
- adc_env : app_adc_params_t
- adc_get_trim_func : _hal_adc_callback
- adc_msp_deinit : _hal_adc_callback
- adc_msp_init : _hal_adc_callback
- adc_state : adc_env_t
- adc_temp : adc_trim_info_t
- add_credits_cplt : ble_l2cap_evt_t
- add_credits_ind : ble_l2cap_evt_t
- addr : _xqspi_command_t , ble_gap_addr_t
- addr_size : _xqspi_command_t
- addr_type : ble_gap_bdaddr_t , ble_gap_evt_peer_name_get_t
- address : _qspi_command_t , app_graphics_dc_cmd_t
- address_size : _ll_qspi_init_t , _qspi_command_t
- address_width : app_graphics_dc_cmd_t
- addressing_mode : _i2c_init
- adv_addr : ble_gap_per_sync_param_t
- adv_hdl : iso_set_per_adv_set_info_tran_t
- adv_idx : iso_start_bd_ann_t , iso_start_gen_ann_t , iso_start_target_ann_t
- adv_info : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t
- adv_intv_max : ble_gap_adv_param_t , ble_gap_adv_period_cfg_t , ble_gap_adv_prim_cfg_t
- adv_intv_min : ble_gap_adv_param_t , ble_gap_adv_period_cfg_t , ble_gap_adv_prim_cfg_t
- adv_mode : ble_gap_adv_param_t
- adv_param : thscps_evt_t
- adv_report : ble_gapm_evt_t
- adv_sid : ble_gap_adv_second_cfg_t , ble_gap_evt_adv_report_t , ble_gap_evt_sync_established_t , ble_gap_ext_adv_report_ind_t , ble_gap_period_adv_addr_cfg_t , ble_gap_sync_established_ind_t , iso_per_adv_sync_tran_rcv_evt_t
- adv_stop : ble_gapm_evt_t
- adv_tx_power : ble_gap_dev_info_t
- adv_type : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t , iso_start_target_ann_t
- aes_done_callback : _hal_aes_callback
- aes_env : app_aes_params_t
- aes_error_callback : _hal_aes_callback
- aes_mask : _keyram_mask
- aes_msp_deinit : _hal_aes_callback
- aes_msp_init : _hal_aes_callback
- aes_state : aes_env_t
- ags_alexa_stream_cb : ags_init_t
- ags_control_stream_cb : ags_init_t
- alarm : _calendar_handle , _rtc_handle_t
- alarm_counter : _aon_wdt_init
- alarm_date_week_mask : _calendar_alarm
- alarm_sel : _calendar_alarm
- alert_level : ias_evt_t , lls_c_evt_t , lls_evt_t
- alert_num : ans_c_new_alert_t , ans_new_alert_t
- alert_status : pass_c_evt_t , pass_init_t
- align : _ll_pwm_init_t , pwm_init_t
- alpha : __hal_gdc_layer_t , app_graphics_dc_framelayer_t
- ams_attr_display_handle : ams_c_handles_t
- ams_attr_update_cccd_handle : ams_c_handles_t
- ams_attr_update_handle : ams_c_handles_t
- ams_cmd_cccd_handle : ams_c_handles_t
- ams_cmd_handle : ams_c_handles_t
- ams_srvc_end_handle : ams_c_handles_t
- ams_srvc_start_handle : ams_c_handles_t
- ancs_control_point_handle : ancs_c_att_handles_t
- ancs_data_source_cccd_handle : ancs_c_att_handles_t
- ancs_data_source_handle : ancs_c_att_handles_t
- ancs_ntf_source_cccd_handle : ancs_c_att_handles_t
- ancs_ntf_source_handle : ancs_c_att_handles_t
- ancs_service_handle : ancs_c_att_handles_t
- ann_status : cgms_get_info_req_t , cgms_meas_rec_t
- ans_ctrl_pt_handle : ans_c_handles_t
- ans_new_alert_cccd_handle : ans_c_handles_t
- ans_new_alert_handle : ans_c_handles_t
- ans_srvc_end_handle : ans_c_handles_t
- ans_srvc_start_handle : ans_c_handles_t
- ans_sup_new_alert_cat_handle : ans_c_handles_t
- ans_sup_unread_alert_cat_handle : ans_c_handles_t
- ans_unread_alert_cccd_handle : ans_c_handles_t
- ans_unread_alert_handle : ans_c_handles_t
- antenna_id : ble_gap_connless_iq_sample_param_t , ble_gap_set_conn_cte_rcv_param_t , ble_gap_set_conn_cte_trans_param_t , gap_connless_cte_trans_param_t
- antenna_num : ble_gap_connless_iq_sample_param_t
- antennae_num : ble_gap_antenna_inf_t
- aon_aon_wdt_env : app_aon_wdt_params_t
- aon_gpio_callback : _hal_aon_gpio_callback
- aon_wdt_alarm_callback : _hal_aon_wdt_callback
- aon_wdt_state : aon_aon_wdt_env_t
- app_prepare_for_sleep : app_sleep_callbacks_t
- app_wake_up_ind : app_sleep_callbacks_t
- appearance : ble_gapc_set_dev_info_t
- arg : app_io_evt_t
- assert_err_cb : sys_assert_cb_t
- assert_param_cb : sys_assert_cb_t
- assert_warn_cb : sys_assert_cb_t
- ate_version : _efuse_trim0_t
- att_idx : ras_ad_send_nti_ind_cmp_info_t
- attr : ble_gattc_browse_attr_info
- attr_char : ble_gattc_browse_attr_info
- attr_count : ams_c_ett_attr_id_t
- attr_hdl : ble_gattc_desc_t , ble_gattc_include_t
- attr_id : ams_c_attr_info_t , ams_c_ett_attr_id_t
- attr_info : ams_c_evt_t
- attr_tab : ble_gatts_create_db_t
- attr_tab_128 : ble_gatts_create_db_t::attribute_table
- attr_tab_16 : ble_gatts_create_db_t::attribute_table
- attr_tab_cfg : ble_gatts_create_db_t
- attr_tab_type : ble_gatts_create_db_t
- attr_type : attr_cache_info_t , ble_gattc_browse_attr_char_t , ble_gattc_browse_attr_info , ble_gattc_browse_attr_t , ble_gattc_browse_inc_srvc_t
- audio_freq : _i2s_init , _ll_i2s_init_t
- auth : ble_sec_evt_enc_ind_t , ble_sec_param_t
- auth_code_len : bms_init_t
- auth_code_val : bms_init_t
- auto_reload : _dual_timer_init , _ll_dual_timer_init , _ll_timer_init_t , _timer_init
- average_val : thscps_test_info_t