Macros
Service and Characteristics UUID
BLE Services » Multi Link Multi Role Service Client (MLMR_C) » Defines
Collaboration diagram for Service and Characteristics UUID:

## Macros
#define | MLMR_C_SVC_UUID
| UUID of MLMR_C Service. More...
#define | MLMR_C_TX_CHAR_UUID
| UUID of MLMR_C Tx characterisitc. More...
#define | MLMR_C_RX_CHAR_UUID
| UUID of MLMR_C Rx characterisitc. More...
#define | MLMR_C_FLOW_CTRL_UUID
| UUID of MLMR_C Flow Control characterisitc. More...

## Detailed Description

## Macro Definition Documentation

## ◆ MLMR_C_FLOW_CTRL_UUID

#define MLMR_C_FLOW_CTRL_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x04, 0x02, 0xED, 0xA6}

UUID of MLMR_C Flow Control characterisitc.

Definition at line 85 of file mlmr_c.h.

## ◆ MLMR_C_RX_CHAR_UUID

#define MLMR_C_RX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x03, 0x02, 0xED, 0xA6}

UUID of MLMR_C Rx characterisitc.

Definition at line 83 of file mlmr_c.h.

## ◆ MLMR_C_SVC_UUID

#define MLMR_C_SVC_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x02, 0xED, 0xA6}

UUID of MLMR_C Service.

Definition at line 79 of file mlmr_c.h.

## ◆ MLMR_C_TX_CHAR_UUID

#define MLMR_C_TX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x02, 0x02, 0xED, 0xA6}

UUID of MLMR_C Tx characterisitc.

Definition at line 81 of file mlmr_c.h.