Macros
PWM period unit default configuretion
Peripheral Driver » LL Driver » PWM » Defines » PWM Exported Constants
Collaboration diagram for PWM period unit default configuretion:

## Macros
#define | LL_PWM_PRESCALER_UNIT (128)
| The unit of prescaler is 128. More...
#define | LL_PWM_BREATH_PRESCALER_UNIT (128)
| The unit of breath prescaler is 128. More...
#define | LL_PWM_HOLD_PRESCALER_UNIT (10)
| The unit of hold prescaler is 10. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWM_BREATH_PRESCALER_UNIT

#define LL_PWM_BREATH_PRESCALER_UNIT (128)

The unit of breath prescaler is 128.

Definition at line 191 of file gr55xx_ll_pwm.h.

## ◆ LL_PWM_HOLD_PRESCALER_UNIT

#define LL_PWM_HOLD_PRESCALER_UNIT (10)

The unit of hold prescaler is 10.

Definition at line 192 of file gr55xx_ll_pwm.h.

## ◆ LL_PWM_PRESCALER_UNIT

#define LL_PWM_PRESCALER_UNIT (128)

The unit of prescaler is 128.

Definition at line 190 of file gr55xx_ll_pwm.h.