Enumerations
Enumerations
Peripheral Driver » HAL Driver » RTC
Collaboration diagram for Enumerations:

## Enumerations
enum | hal_rtc_state_t { HAL_RTC_READY = 0x00U, HAL_RTC_RESET, HAL_RTC_RUNNING, HAL_RTC_ERROR }
| hal_rtc_state definition More...
enum | rtc_tick_state_t { TICK_READY = 0x00U, TICK_RUNNING, TICK_ERROR }
| rtc_tick_state definition More...
enum | rtc_alarm_state_t { ALARM_READY = 0x00U, ALARM_RUNNING, ALARM_ERROR }
| rtc_alarm_state definition More...
enum | overflow_det_t { CLOSED = 0x00U, OPENED = !CLOSED }
| overflow config More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_rtc_state_t

enum hal_rtc_state_t

hal_rtc_state definition

Enumerator
HAL_RTC_READY |
HAL_RTC_RESET |
HAL_RTC_RUNNING |
HAL_RTC_ERROR |

Definition at line 186 of file gr55xx_hal_rtc.h.

## ◆ overflow_det_t

enum overflow_det_t

overflow config

Enumerator
CLOSED |
OPENED |

Definition at line 217 of file gr55xx_hal_rtc.h.

## ◆ rtc_alarm_state_t

enum rtc_alarm_state_t

rtc_alarm_state definition

Enumerator
ALARM_READY |
ALARM_RUNNING |
ALARM_ERROR |

Definition at line 207 of file gr55xx_hal_rtc.h.

## ◆ rtc_tick_state_t

enum rtc_tick_state_t

rtc_tick_state definition

Enumerator
TICK_READY |
TICK_RUNNING |
TICK_ERROR |

Definition at line 197 of file gr55xx_hal_rtc.h.