Functions
Initialization and de-initialization functions
Peripheral Driver » HAL Driver » AON_WDT » Functions

Initialization and Configuration functions. More...

Collaboration diagram for Initialization and de-initialization functions:

## Functions
hal_status_t | hal_aon_wdt_init (aon_wdt_handle_t *p_aon_wdt)
| Initialize the AON_WDT according to the specified parameters in the wdt_init_t of associated handle. More...
hal_status_t | hal_aon_wdt_deinit (aon_wdt_handle_t *p_aon_wdt)
| De-initialize the AON_WDT peripheral. More...

## Detailed Description

Initialization and Configuration functions.

      ==============================================================================
              ##### Initialization and Configuration functions #####
      ==============================================================================
      [..]
        This section provides functions allowing to:
          (+) Initialize and start the AON_WDT according to the specified parameters
              in the wdt_init_t of associated handle.
          (+) Initialize the AON_WDT MSP.

## Function Documentation

## ◆ hal_aon_wdt_deinit()

hal_status_t hal_aon_wdt_deinit | ( | aon_wdt_handle_t * | p_aon_wdt | ) |

De-initialize the AON_WDT peripheral.

Parameters

  [in] | p_aon_wdt | AON_WDT handle.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.

## ◆ hal_aon_wdt_init()

hal_status_t hal_aon_wdt_init | ( | aon_wdt_handle_t * | p_aon_wdt | ) |

Initialize the AON_WDT according to the specified parameters in the wdt_init_t of associated handle.

Parameters

  [in] | p_aon_wdt | Pointer to a AON_WDT handle which contains the configuration information for the specified AON_WDT module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.