Enumerations
HAL TIMER state
Peripheral Driver » HAL Driver » TIMER » Enumerations
Collaboration diagram for HAL TIMER state:

## Enumerations
enum | hal_timer_state_t { HAL_TIMER_STATE_RESET = 0x00, HAL_TIMER_STATE_READY = 0x01, HAL_TIMER_STATE_BUSY = 0x02, HAL_TIMER_STATE_ERROR = 0x04 }
| HAL TIMER State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_timer_state_t

enum hal_timer_state_t

HAL TIMER State Enumerations definition.

Enumerator
HAL_TIMER_STATE_RESET | Peripheral not yet initialized or disabled
HAL_TIMER_STATE_READY | Peripheral Initialized and ready for use
HAL_TIMER_STATE_BUSY | An internal process is ongoing
HAL_TIMER_STATE_ERROR | Reception process is ongoing

Definition at line 75 of file gr55xx_hal_tim.h.