Public Attributes | List of all members
iso_set_cig_param_cmpl_evt_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for set cig parameter complete event. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | status
| 0x00: succeeded. More...
uint8_t | cig_id
| Used to identify a CIG, (Range: 0x00 to 0xEF). More...
uint8_t | cis_count
| Total number of CISs, (Range: 0x00 to 0x10). More...
uint16_t * | cis_hdl
| List of connection handles of CISs in the CIG, (Range: 0x0000 to 0x0EFF). More...

## Detailed Description

The parameter for set cig parameter complete event.

Definition at line 589 of file ble_iso.h.

## Member Data Documentation

## ◆ cig_id

uint8_t iso_set_cig_param_cmpl_evt_t::cig_id

Used to identify a CIG, (Range: 0x00 to 0xEF).

Definition at line 592 of file ble_iso.h.

## ◆ cis_count

uint8_t iso_set_cig_param_cmpl_evt_t::cis_count

Total number of CISs, (Range: 0x00 to 0x10).

Definition at line 593 of file ble_iso.h.

## ◆ cis_hdl

uint16_t* iso_set_cig_param_cmpl_evt_t::cis_hdl

List of connection handles of CISs in the CIG, (Range: 0x0000 to 0x0EFF).

Definition at line 594 of file ble_iso.h.

## ◆ status

uint8_t iso_set_cig_param_cmpl_evt_t::status

0x00: succeeded.

0x01-0xFF: failed

Definition at line 591 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h