Enumerations
Enumerations
Peripheral Driver » APP DRIVER » OSPI
Collaboration diagram for Enumerations:

## Enumerations
enum | app_ospi_clock_freq_e { OSPI_CLOCK_FREQ_48MHz = 0x00, OSPI_CLOCK_FREQ_32MHz = 0x01, OSPI_CLOCK_FREQ_24MHz = 0x02, OSPI_CLOCK_FREQ_16MHz = 0x03 }
| OSPI Clock Frequency Enumerations definition. More...
enum | app_ospi_phy_delay_e { OSPI_PHY_DELAY_TAP_2 = 0x01, OSPI_PHY_DELAY_TAP_3 = 0x02, OSPI_PHY_DELAY_TAP_4 = 0x03 }
| OSPI PHY Delay Value Enumerations definition. More...
enum | app_ospi_psram_drv_strength_e { OSPI_PSRAM_DRV_STR_FULL = 0x00, OSPI_PSRAM_DRV_STR_HALF = 0x01, OSPI_PSRAM_DRV_STR_ONE_FORTH = 0x02, OSPI_PSRAM_DRV_STR_ONE_EIGHTH = 0x03 }
| PSRAM Drive Strength Enumerations definition. More...
enum | app_ospi_psram_rd_latency_e { OSPI_PSRAM_RD_LATENCY_3 = 0x00, OSPI_PSRAM_RD_LATENCY_4 = 0x01, OSPI_PSRAM_RD_LATENCY_5 = 0x02, OSPI_PSRAM_RD_LATENCY_6 = 0x03, OSPI_PSRAM_RD_LATENCY_7 = 0x04 }
| PSRAM Read Latency Enumerations definition. More...
enum | app_ospi_psram_wr_latency_e { OSPI_PSRAM_WR_LATENCY_3 = 0x00, OSPI_PSRAM_WR_LATENCY_4 = 0x04, OSPI_PSRAM_WR_LATENCY_5 = 0x02, OSPI_PSRAM_WR_LATENCY_6 = 0x06, OSPI_PSRAM_WR_LATENCY_7 = 0x01 }
| PSRAM Write Latency Enumerations definition. More...
enum | app_ospi_access_mode_e { OSPI_ACCESS_MEMORY = 0, OSPI_ACCESS_REGISTER, OSPI_ACCESS_UNSET }
| PSRAM Access Mode Enumerations definition. More...
enum | app_ospi_work_state_e { OSPI_STATE_DEEP_SLEEP = 0, OSPI_STATE_HALF_SLEEP = 1, OSPI_STATE_ACTIVE = 2 }
| PSRAM Work Mode Enumerations definition. More...
enum | app_ospi_pasr_e { OSPI_PASR_FULL = 0x00, OSPI_PASR_BOTTOM_4MB = 0x01, OSPI_PASR_BOTTOM_2MB = 0x02, OSPI_PASR_BOTTOM_1MB = 0x03, OSPI_PASR_NONE = 0x04, OSPI_PASR_TOP_4MB = 0x05, OSPI_PASR_TOP_2MB = 0x06, OSPI_PASR_TOP_1MB = 0x07, OSPI_PASR_MAX }
| PSRAM Partial Array Refresh Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ app_ospi_access_mode_e

enum app_ospi_access_mode_e

PSRAM Access Mode Enumerations definition.

Enumerator
OSPI_ACCESS_MEMORY |
OSPI_ACCESS_REGISTER |
OSPI_ACCESS_UNSET |

Definition at line 124 of file app_graphics_ospi.h.

## ◆ app_ospi_clock_freq_e

enum app_ospi_clock_freq_e

OSPI Clock Frequency Enumerations definition.

Enumerator
OSPI_CLOCK_FREQ_48MHz |
OSPI_CLOCK_FREQ_32MHz |
OSPI_CLOCK_FREQ_24MHz |
OSPI_CLOCK_FREQ_16MHz |

Definition at line 72 of file app_graphics_ospi.h.

## ◆ app_ospi_pasr_e

enum app_ospi_pasr_e

PSRAM Partial Array Refresh Enumerations definition.

Enumerator
OSPI_PASR_FULL |
OSPI_PASR_BOTTOM_4MB |
OSPI_PASR_BOTTOM_2MB |
OSPI_PASR_BOTTOM_1MB |
OSPI_PASR_NONE |
OSPI_PASR_TOP_4MB |
OSPI_PASR_TOP_2MB |
OSPI_PASR_TOP_1MB |
OSPI_PASR_MAX |

Definition at line 142 of file app_graphics_ospi.h.

## ◆ app_ospi_phy_delay_e

enum app_ospi_phy_delay_e

OSPI PHY Delay Value Enumerations definition.

Enumerator
OSPI_PHY_DELAY_TAP_2 |
OSPI_PHY_DELAY_TAP_3 |
OSPI_PHY_DELAY_TAP_4 |

Definition at line 83 of file app_graphics_ospi.h.

## ◆ app_ospi_psram_drv_strength_e

enum app_ospi_psram_drv_strength_e

PSRAM Drive Strength Enumerations definition.

Enumerator
OSPI_PSRAM_DRV_STR_FULL |
OSPI_PSRAM_DRV_STR_HALF |
OSPI_PSRAM_DRV_STR_ONE_FORTH |
OSPI_PSRAM_DRV_STR_ONE_EIGHTH |

Definition at line 92 of file app_graphics_ospi.h.

## ◆ app_ospi_psram_rd_latency_e

enum app_ospi_psram_rd_latency_e

PSRAM Read Latency Enumerations definition.

Enumerator
OSPI_PSRAM_RD_LATENCY_3 |
OSPI_PSRAM_RD_LATENCY_4 |
OSPI_PSRAM_RD_LATENCY_5 |
OSPI_PSRAM_RD_LATENCY_6 |
OSPI_PSRAM_RD_LATENCY_7 |

Definition at line 102 of file app_graphics_ospi.h.

## ◆ app_ospi_psram_wr_latency_e

enum app_ospi_psram_wr_latency_e

PSRAM Write Latency Enumerations definition.

Enumerator
OSPI_PSRAM_WR_LATENCY_3 |
OSPI_PSRAM_WR_LATENCY_4 |
OSPI_PSRAM_WR_LATENCY_5 |
OSPI_PSRAM_WR_LATENCY_6 |
OSPI_PSRAM_WR_LATENCY_7 |

Definition at line 113 of file app_graphics_ospi.h.

## ◆ app_ospi_work_state_e

enum app_ospi_work_state_e

PSRAM Work Mode Enumerations definition.

Enumerator
OSPI_STATE_DEEP_SLEEP |
OSPI_STATE_HALF_SLEEP |
OSPI_STATE_ACTIVE |

Definition at line 133 of file app_graphics_ospi.h.