Macros
QSPI Frame Format
Peripheral Driver » LL Driver » XQSPI » Defines » XQSPI Exported Constants
Collaboration diagram for QSPI Frame Format:

## Macros
#define | LL_XQSPI_QSPI_FRF_SPI 0x00000000UL
| SPI frame format for transfer More...
#define | LL_XQSPI_QSPI_FRF_DUALSPI (2UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)
| Dual-SPI frame format for transfer. More...
#define | LL_XQSPI_QSPI_FRF_QUADSPI (3UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)
| Quad-SPI frame format for transfer. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_QSPI_FRF_DUALSPI

#define LL_XQSPI_QSPI_FRF_DUALSPI (2UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)

Dual-SPI frame format for transfer.

Definition at line 275 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_FRF_QUADSPI

#define LL_XQSPI_QSPI_FRF_QUADSPI (3UL << XQSPI_QSPI_AUXCTRL_QMODE_Pos)

Quad-SPI frame format for transfer.

Definition at line 276 of file gr55xx_ll_xqspi.h.

## ◆ LL_XQSPI_QSPI_FRF_SPI

#define LL_XQSPI_QSPI_FRF_SPI 0x00000000UL

SPI frame format for transfer

Definition at line 274 of file gr55xx_ll_xqspi.h.