Macros
USB interrupt clear
Peripheral Driver » HAL Driver » USB » Defines » USB Exported Constants
Collaboration diagram for USB interrupt clear:

## Macros
#define | USB_IT_CLR_ALL LL_USB_INT_CLR_ALL
| USB all interrupt clear More...
#define | USB_IT_CLR_SUSPEND LL_USB_INT_CLR_SUSPEND
| USB suspend status interrupt clear More...
#define | USB_IT_CLR_EP0_OUT_READY LL_USB_INT_CLR_EP0_OUT_READY
| USB ep0 data out ready interrupt clear More...
#define | USB_IT_CLR_EP1_OUT_READY LL_USB_INT_CLR_EP1_OUT_READY
| USB ep1 data out ready interrupt clear More...
#define | USB_IT_CLR_CRC16_ERR LL_USB_INT_CLR_CRC16_ERR
| USB receive CRC error data interrupt clear More...
#define | USB_IT_CLR_UPID_ERR LL_USB_INT_CLR_UPID_ERR
| USB receive unsupported PID interrupt clear More...
#define | USB_IT_CLR_TIMEOUT_ERR LL_USB_INT_CLR_TIMEOUT_ERR
| USB rx/tx timeout error interrupt clear More...
#define | USB_IT_CLR_SEQ_ERR LL_USB_INT_CLR_SEQ_ERR
| USB DATA0/DATA1 PID sequence error interrupt clear More...
#define | USB_IT_CLR_PID_CKS_ERR LL_USB_INT_CLR_PID_CKS_ERR
| USB PID checksum error interrupt clear More...
#define | USB_IT_CLR_PID_CRC_ERR LL_USB_INT_CLR_PID_CRC_ERR
| USB PID CRC error interrupt clear More...
#define | USB_IT_CLR_HOST_RESET LL_USB_INT_CLR_HOST_RESET
| USB host reset interrupt clear More...
#define | USB_IT_CLR_AHB_XFER_ERR LL_USB_INT_CLR_AHB_XFER_ERR
| USB ep3 and ep4 AHB master receive error interrupt clear More...
#define | USB_IT_CLR_NSE_ERR LL_USB_INT_CLR_NSE_ERR
| USB no such endpoint error interrupt clear More...
#define | USB_IT_CLR_EP3_AHB_XFER_DONE LL_USB_INT_CLR_EP3_AHB_XFER_DONE
| USB ep3 AHB master transfer done interrupt clear More...
#define | USB_IT_CLR_SYNC_ERR LL_USB_INT_CLR_SYNC_ERR
| USB SYNC error interrupt clear More...
#define | USB_IT_CLR_BIT_STUFF_ERR LL_USB_INT_CLR_BIT_STUFF_ERR
| USB bit stuff error interrupt clear More...
#define | USB_IT_CLR_BYTE_ERR LL_USB_INT_CLR_BYTE_ERR
| USB byte error interrupt clear More...
#define | USB_IT_CLR_SOF LL_USB_INT_CLR_SOF
| USB SOF interrupt clear More...
#define | USB_IT_CLR_EP0_TX_DONE LL_USB_INT_CLR_EP0_TX_DONE
| USB ep0 TX done interrupt clear More...
#define | USB_IT_CLR_EP2_TX_DONE LL_USB_INT_CLR_EP2_TX_DONE
| USB ep2 TX done interrupt clear More...
#define | USB_IT_CLR_EP3_TX_DONE LL_USB_INT_CLR_EP3_TX_DONE
| USB ep3 TX done interrupt clear More...
#define | USB_IT_CLR_INTO_CONFIG LL_USB_INT_CLR_INTO_CONFIG
| USB into cofig status interrupt clear More...
#define | USB_IT_CLR_EP5_OUT_READY LL_USB_INT_CLR_EP5_OUT_READY
| USB ep5 data out ready interrupt clear More...
#define | USB_IT_CLR_EP4_AHB_XFER_DONE LL_USB_INT_CLR_EP4_AHB_XFER_DONE
| USB ep4 AHB master transfer done interrupt clear More...
#define | USB_IT_CLR_EP4_TX_DONE LL_USB_INT_CLR_EP4_TX_DONE
| USB ep4 TX done interrupt clear More...
#define | USB_IT_CLR_EP5_AHB_XFER_DONE LL_USB_INT_CLR_EP5_AHB_XFER_DONE
| USB ep5 AHB master transfer done interrupt clear More...
#define | USB_IT_CLR_EP5_TIMER_OUT_ERR LL_USB_INT_CLR_EP5_TIMER_OUT_ERR
| USB ep5 timer out error interrupt clear More...

## Detailed Description

## Macro Definition Documentation

## ◆ USB_IT_CLR_AHB_XFER_ERR

#define USB_IT_CLR_AHB_XFER_ERR LL_USB_INT_CLR_AHB_XFER_ERR

USB ep3 and ep4 AHB master receive error interrupt clear

Definition at line 408 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_ALL

#define USB_IT_CLR_ALL LL_USB_INT_CLR_ALL

USB all interrupt clear

Definition at line 397 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_BIT_STUFF_ERR

#define USB_IT_CLR_BIT_STUFF_ERR LL_USB_INT_CLR_BIT_STUFF_ERR

USB bit stuff error interrupt clear

Definition at line 412 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_BYTE_ERR

#define USB_IT_CLR_BYTE_ERR LL_USB_INT_CLR_BYTE_ERR

USB byte error interrupt clear

Definition at line 413 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_CRC16_ERR

#define USB_IT_CLR_CRC16_ERR LL_USB_INT_CLR_CRC16_ERR

USB receive CRC error data interrupt clear

Definition at line 401 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP0_OUT_READY

#define USB_IT_CLR_EP0_OUT_READY LL_USB_INT_CLR_EP0_OUT_READY

USB ep0 data out ready interrupt clear

Definition at line 399 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP0_TX_DONE

#define USB_IT_CLR_EP0_TX_DONE LL_USB_INT_CLR_EP0_TX_DONE

USB ep0 TX done interrupt clear

Definition at line 415 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP1_OUT_READY

#define USB_IT_CLR_EP1_OUT_READY LL_USB_INT_CLR_EP1_OUT_READY

USB ep1 data out ready interrupt clear

Definition at line 400 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP2_TX_DONE

#define USB_IT_CLR_EP2_TX_DONE LL_USB_INT_CLR_EP2_TX_DONE

USB ep2 TX done interrupt clear

Definition at line 416 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP3_AHB_XFER_DONE

#define USB_IT_CLR_EP3_AHB_XFER_DONE LL_USB_INT_CLR_EP3_AHB_XFER_DONE

USB ep3 AHB master transfer done interrupt clear

Definition at line 410 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP3_TX_DONE

#define USB_IT_CLR_EP3_TX_DONE LL_USB_INT_CLR_EP3_TX_DONE

USB ep3 TX done interrupt clear

Definition at line 417 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP4_AHB_XFER_DONE

#define USB_IT_CLR_EP4_AHB_XFER_DONE LL_USB_INT_CLR_EP4_AHB_XFER_DONE

USB ep4 AHB master transfer done interrupt clear

Definition at line 420 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP4_TX_DONE

#define USB_IT_CLR_EP4_TX_DONE LL_USB_INT_CLR_EP4_TX_DONE

USB ep4 TX done interrupt clear

Definition at line 421 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP5_AHB_XFER_DONE

#define USB_IT_CLR_EP5_AHB_XFER_DONE LL_USB_INT_CLR_EP5_AHB_XFER_DONE

USB ep5 AHB master transfer done interrupt clear

Definition at line 422 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP5_OUT_READY

#define USB_IT_CLR_EP5_OUT_READY LL_USB_INT_CLR_EP5_OUT_READY

USB ep5 data out ready interrupt clear

Definition at line 419 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_EP5_TIMER_OUT_ERR

#define USB_IT_CLR_EP5_TIMER_OUT_ERR LL_USB_INT_CLR_EP5_TIMER_OUT_ERR

USB ep5 timer out error interrupt clear

Definition at line 423 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_HOST_RESET

#define USB_IT_CLR_HOST_RESET LL_USB_INT_CLR_HOST_RESET

USB host reset interrupt clear

Definition at line 407 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_INTO_CONFIG

#define USB_IT_CLR_INTO_CONFIG LL_USB_INT_CLR_INTO_CONFIG

USB into cofig status interrupt clear

Definition at line 418 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_NSE_ERR

#define USB_IT_CLR_NSE_ERR LL_USB_INT_CLR_NSE_ERR

USB no such endpoint error interrupt clear

Definition at line 409 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_PID_CKS_ERR

#define USB_IT_CLR_PID_CKS_ERR LL_USB_INT_CLR_PID_CKS_ERR

USB PID checksum error interrupt clear

Definition at line 405 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_PID_CRC_ERR

#define USB_IT_CLR_PID_CRC_ERR LL_USB_INT_CLR_PID_CRC_ERR

USB PID CRC error interrupt clear

Definition at line 406 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_SEQ_ERR

#define USB_IT_CLR_SEQ_ERR LL_USB_INT_CLR_SEQ_ERR

USB DATA0/DATA1 PID sequence error interrupt clear

Definition at line 404 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_SOF

#define USB_IT_CLR_SOF LL_USB_INT_CLR_SOF

USB SOF interrupt clear

Definition at line 414 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_SUSPEND

#define USB_IT_CLR_SUSPEND LL_USB_INT_CLR_SUSPEND

USB suspend status interrupt clear

Definition at line 398 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_SYNC_ERR

#define USB_IT_CLR_SYNC_ERR LL_USB_INT_CLR_SYNC_ERR

USB SYNC error interrupt clear

Definition at line 411 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_TIMEOUT_ERR

#define USB_IT_CLR_TIMEOUT_ERR LL_USB_INT_CLR_TIMEOUT_ERR

USB rx/tx timeout error interrupt clear

Definition at line 403 of file gr55xx_hal_usb.h.

## ◆ USB_IT_CLR_UPID_ERR

#define USB_IT_CLR_UPID_ERR LL_USB_INT_CLR_UPID_ERR

USB receive unsupported PID interrupt clear

Definition at line 402 of file gr55xx_hal_usb.h.