Macros
QSPI Address and Instruction Transfer Format
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for QSPI Address and Instruction Transfer Format:

## Macros
#define | LL_QSPI_INST_ADDR_ALL_IN_SPI 0x00000000UL
| Instruction and address are sent in SPI mode. More...
#define | LL_QSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1UL << QSPI_SCTRL0_TRANSTYPE_Pos)
| Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode. More...
#define | LL_QSPI_INST_ADDR_ALL_IN_SPIFRF (2UL << QSPI_SCTRL0_TRANSTYPE_Pos)
| Instruction and address are sent in Daul/Quad SPI mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_INST_ADDR_ALL_IN_SPI

#define LL_QSPI_INST_ADDR_ALL_IN_SPI 0x00000000UL

Instruction and address are sent in SPI mode.

Definition at line 555 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_INST_ADDR_ALL_IN_SPIFRF

#define LL_QSPI_INST_ADDR_ALL_IN_SPIFRF (2UL << QSPI_SCTRL0_TRANSTYPE_Pos)

Instruction and address are sent in Daul/Quad SPI mode.

Definition at line 557 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_INST_IN_SPI_ADDR_IN_SPIFRF

#define LL_QSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1UL << QSPI_SCTRL0_TRANSTYPE_Pos)

Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode.

Definition at line 556 of file gr55xx_ll_qspi.h.