Macros
Block1 Clock During WFI
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants
Collaboration diagram for Block1 Clock During WFI:

## Macros
#define | LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK
| Hclk for Always-on register More...
#define | LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK
| Hclk for cache top More...
#define | LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK
| Hclk for SRAMs More...
#define | LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)
| All clock group 1 More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_WFI_ALL_HCLK1

#define LL_CGC_WFI_ALL_HCLK1 ((uint32_t)0x00000007U)

All clock group 1

Definition at line 95 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_AON_MCUSUB_HCLK

#define LL_CGC_WFI_AON_MCUSUB_HCLK MCU_SUB_WFI_AON_MCUSUB_HCLK

Hclk for Always-on register

Definition at line 91 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_SRAM_HCLK

#define LL_CGC_WFI_SRAM_HCLK MCU_SUB_WFI_SRAM_HCLK

Hclk for SRAMs

Definition at line 93 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_WFI_XF_XQSPI_HCLK

#define LL_CGC_WFI_XF_XQSPI_HCLK MCU_SUB_WFI_XF_XQSPI_HCLK

Hclk for cache top

Definition at line 92 of file gr55xx_ll_cgc.h.