Here is a list of all file members with links to the files they belong to:

### - p -

- p_device_resume_func : gr55xx_hal_pwr_mgmt.h
- p_device_suspend_func : gr55xx_hal_pwr_mgmt.h
- PACK_INT : ble_iso.h
- PACK_SEQ : ble_iso.h
- package : gr55xx_efuse_layout.h
- PACKAGE_GR5526_DEBUG : gr55xx_sys_sdk.h
- PACKAGE_GR5526RGNI : gr55xx_sys_sdk.h
- PACKAGE_GR5526RGNIP : gr55xx_sys_sdk.h
- PACKAGE_GR5526RJNIP : gr55xx_sys_sdk.h
- PACKAGE_GR5526VGBI : gr55xx_sys_sdk.h
- PACKAGE_GR5526VGBIP : gr55xx_sys_sdk.h
- PACKAGE_NONE : gr55xx_sys_sdk.h
- package_type_t : gr55xx_sys_sdk.h
- PARAM_ID : nvds_tag.h
- PARAM_ID_ACTCLK_DRIFT : nvds_tag.h
- PARAM_ID_ACTIVITY_MOVE_CONFIG : nvds_tag.h
- PARAM_ID_BD_ADDRESS : nvds_tag.h
- PARAM_ID_CH_ASS_EN : nvds_tag.h
- PARAM_ID_DEVICE_NAME : nvds_tag.h
- PARAM_ID_DFT_SLAVE_MD : nvds_tag.h
- PARAM_ID_DIAG_BLE_HW : nvds_tag.h
- PARAM_ID_DIAG_DM_HW : nvds_tag.h
- PARAM_ID_DIAG_PLF : nvds_tag.h
- PARAM_ID_DIAG_SW : nvds_tag.h
- PARAM_ID_GDX_ADV_INT : nvds_tag.h
- PARAM_ID_LE_CODED_PHY_500 : nvds_tag.h
- PARAM_ID_LPCLK_DRIFT : nvds_tag.h
- PARAM_ID_RF_BTIPT_GAIN_SETTING : nvds_tag.h
- PARAM_ID_RF_BTIPT_VERSION : nvds_tag.h
- PARAM_ID_RF_BTIPT_XO_SETTING : nvds_tag.h
- PARAM_ID_RF_XO_OFFSET : nvds_tag.h
- PARAM_ID_RSSI_HIGH_THR : nvds_tag.h
- PARAM_ID_RSSI_INTERF_THR : nvds_tag.h
- PARAM_ID_RSSI_LOW_THR : nvds_tag.h
- PARAM_ID_SCAN_EXT_ADV : nvds_tag.h
- PARAM_ID_SCHED_SCAN_DUR : nvds_tag.h
- PARAM_ID_TRACER_CONFIG : nvds_tag.h
- pass_alert_status_set() : pass.h
- PASS_ALERT_STATUS_VAL_LEN : pass.h
- PASS_ALL_STATE_ACTIVE : pass.h
- pass_c_alert_status_notify_set() : pass_c.h
- pass_c_alert_status_read() : pass_c.h
- PASS_C_ALL_STATE_ACTIVE : pass_c.h
- PASS_C_CONNECTION_MAX : pass_c.h
- pass_c_ctrl_point_set() : pass_c.h
- PASS_C_CTRL_PT_CANCEL_SLIENT_MODE : pass_c.h
- PASS_C_CTRL_PT_MUTE_ONCE : pass_c.h
- PASS_C_CTRL_PT_SILENT_MODE : pass_c.h
- pass_c_disc_srvc_start() : pass_c.h
- PASS_C_DISPLAY_ALERT_ACTIVE : pass_c.h
- PASS_C_EVT_ALERT_STATUS_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_ALERT_STATUS_RECEIVE : pass_c.h
- PASS_C_EVT_CTRL_POINT_SET_SUCCESS : pass_c.h
- PASS_C_EVT_DISCOVERY_COMPLETE : pass_c.h
- PASS_C_EVT_DISCOVERY_FAIL : pass_c.h
- pass_c_evt_handler_t : pass_c.h
- PASS_C_EVT_INVALID : pass_c.h
- PASS_C_EVT_RINGER_SET_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_RINGER_SET_RECEIVE : pass_c.h
- pass_c_evt_type_t : pass_c.h
- PASS_C_EVT_WRITE_OP_ERR : pass_c.h
- PASS_C_NO_STATE_ACTIVE : pass_c.h
- PASS_C_RINGER_ACTIVE : pass_c.h
- pass_c_ringer_ctrl_pt_t : pass_c.h
- PASS_C_RINGER_CTRL_PT_VAL_LEN : pass_c.h
- PASS_C_RINGER_SET_NORMAL : pass_c.h
- pass_c_ringer_set_notify_set() : pass_c.h
- pass_c_ringer_set_read() : pass_c.h
- PASS_C_RINGER_SET_SILENT : pass_c.h
- PASS_C_VIBRATE_ACTIVE : pass_c.h
- PASS_CHAR_FULL : pass.h
- PASS_CHAR_MANDATORY : pass.h
- PASS_CHAR_RING_CTRL_PT_SUP : pass.h
- pass_client_init() : pass_c.h
- PASS_CONNECTION_MAX : pass.h
- PASS_CTRL_PT_CANCEL_SLIENT_MODE : pass.h
- PASS_CTRL_PT_MUTE_ONCE : pass.h
- PASS_CTRL_PT_SILENT_MODE : pass.h
- PASS_DISPLAY_ALERT_ACTIVE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_DISABLE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_ENABLE : pass.h
- pass_evt_handler_t : pass.h
- PASS_EVT_INVALID : pass.h
- PASS_EVT_MUTE_ONCE_SET : pass.h
- PASS_EVT_RINGER_SET_NTF_DISABLE : pass.h
- PASS_EVT_RINGER_SET_NTF_ENABLE : pass.h
- PASS_EVT_SILENT_MODE_CANCEL : pass.h
- PASS_EVT_SILENT_MODE_SET : pass.h
- pass_evt_type_t : pass.h
- PASS_NO_STATE_ACTIVE : pass.h
- PASS_RINGER_ACTIVE : pass.h
- pass_ringer_ctrl_pt_t : pass.h
- PASS_RINGER_CTRL_PT_VAL_LEN : pass.h
- PASS_RINGER_SET_NORMAL : pass.h
- PASS_RINGER_SET_SILENT : pass.h
- PASS_RINGER_SET_VAL_LEN : pass.h
- pass_ringer_setting_get() : pass.h
- pass_ringer_setting_set() : pass.h
- pass_service_init() : pass.h
- PASS_VIBRATE_ACTIVE : pass.h
- pattern : gr55xx_efuse_layout.h
- PCS_CONNECTION_MAX : pcs.h
- PCS_EVT_DISCONNECTED : pcs.h
- pcs_evt_handler_t : pcs.h
- PCS_EVT_INVALID : pcs.h
- PCS_EVT_PARAM_SET : pcs.h
- PCS_EVT_SETTING_DISABLE : pcs.h
- PCS_EVT_SETTING_ENABLE : pcs.h
- PCS_EVT_TX_DATA_SENT : pcs.h
- PCS_EVT_TX_DISABLE : pcs.h
- PCS_EVT_TX_ENABLE : pcs.h
- pcs_evt_type_t : pcs.h
- PCS_MAX_DATA_LEN : pcs.h
- pcs_service_init() : pcs.h
- PCS_SERVICE_UUID : pcs.h
- PCS_SET_ADV_DATA_10B : pcs.h
- PCS_SET_ADV_DATA_17B : pcs.h
- PCS_SET_ADV_DATA_24B : pcs.h
- PCS_SET_ADV_DATA_31B : pcs.h
- PCS_SET_ADV_DATA_3B : pcs.h
- PCS_SET_PARAM_FAIL : pcs.h
- PCS_SET_PARAM_SUCCESS : pcs.h
- pcs_setting_reply() : pcs.h
- PCS_SETTING_TYPE_ADV_DATA : pcs.h
- PCS_SETTING_TYPE_ADV_INTERVAL : pcs.h
- PCS_SETTING_TYPE_CONN_PARAM : pcs.h
- PCS_SETTING_TYPE_PHY : pcs.h
- pcs_setting_type_t : pcs.h
- PCS_SETTING_TYPE_TX_POWER : pcs.h
- pcs_tx_data_send() : pcs.h
- pdm_handle_t : gr55xx_hal_pdm.h
- pdm_init_t : gr55xx_hal_pdm.h
- PDM_MODE_LEFT : gr55xx_hal_pdm.h
- PDM_MODE_RIGHT : gr55xx_hal_pdm.h
- PDM_MODE_STEREO : gr55xx_hal_pdm.h
- PDM_SAMPLE_RATE_15_625K : gr55xx_hal_pdm.h
- PDM_SAMPLE_RATE_16K : gr55xx_hal_pdm.h
- PDM_SAMPLE_RATE_8K : gr55xx_hal_pdm.h
- PERIPH_DEVICE_NUM_AES : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_DMA0 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_DMA1 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_DSPI : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_HMAC : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C0 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C1 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C2 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C3 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C4 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C5 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2S_M : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2S_S : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_ISO7816 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PDM : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PKC : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM0 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM1 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_QSPI0 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_QSPI1 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_QSPI2 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_RNG : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SNSADC : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIM : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIS : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART0 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART1 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART2 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART3 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART4 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART5 : gr55xx_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_USB : gr55xx_hal_pwr_mgmt.h
- periph_device_number_t : gr55xx_hal_pwr_mgmt.h
- periph_func_t : gr55xx_pwr.h
- periph_state_t : gr55xx_hal_pwr_mgmt.h
- pkc_big_number_add_t : gr55xx_hal_pkc.h
- pkc_big_number_multi_t : gr55xx_hal_pkc.h
- PKC_BIGMULTI_BITS_LENGTH_MAX : gr55xx_hal_pkc.h
- PKC_BITS_LENGTH_MAX : gr55xx_hal_pkc.h
- PKC_BITS_LENGTH_MIN : gr55xx_hal_pkc.h
- pkc_ecc_point_multi_t : gr55xx_hal_pkc.h
- PKC_FLAG_BUSY : gr55xx_hal_pkc.h
- pkc_handle_t : gr55xx_hal_pkc.h
- PKC_IT_DONE : gr55xx_hal_pkc.h
- PKC_IT_ERR : gr55xx_hal_pkc.h
- PKC_IT_OVF : gr55xx_hal_pkc.h
- pkc_modular_add_t : gr55xx_hal_pkc.h
- pkc_modular_compare_t : gr55xx_hal_pkc.h
- pkc_modular_shift_t : gr55xx_hal_pkc.h
- pkc_modular_sub_t : gr55xx_hal_pkc.h
- pkc_montgomery_inversion_t : gr55xx_hal_pkc.h
- pkc_montgomery_multi_t : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_ADD : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_BIGADD : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_BIGMULTI : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_CMP : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_INVER : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_LSHIFT : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_MULTI : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_SUB : gr55xx_hal_pkc.h
- pkc_rsa_modular_exponent_t : gr55xx_hal_pkc.h
- PKC_SECURE_MODE_DISABLE : gr55xx_hal_pkc.h
- PKC_SECURE_MODE_ENABLE : gr55xx_hal_pkc.h
- platform_clock_init_with_rng2() : platform_sdk.h
- platform_clock_init_with_rtc() : platform_sdk.h
- platform_flash_enable_quad() : platform_sdk.h
- platform_init() : platform_sdk.h
- platform_rc_calibration() : platform_sdk.h
- platform_sdk_init() : platform_sdk.h
- PMR_MGMT_ACTIVE_MODE : gr55xx_pwr.h
- PMR_MGMT_FAIL : gr55xx_pwr.h
- PMR_MGMT_IDLE_MODE : gr55xx_pwr.h
- PMR_MGMT_SLEEP_MODE : gr55xx_pwr.h
- PMR_MGMT_SUCCESS : gr55xx_pwr.h
- pmu_calibration_handler() : platform_sdk.h
- POL_SET : gr55xx_ll_gpio.h
- pool_t : tsi_malloc_intern.h
- PRF_CHAR_PRES_FMT_SIZE : ble_prf_types.h
- prf_cli_conf_t : ble_prf_types.h
- PRF_CLI_START_IND : ble_prf_types.h
- PRF_CLI_START_NTF : ble_prf_types.h
- PRF_CLI_STOP_NTFIND : ble_prf_types.h
- prf_error_handler_t : ble_prf_types.h
- prf_find_handle_by_idx() : ble_prf_utils.h
- prf_find_idx_by_handle() : ble_prf_utils.h
- PRF_INVALID_HANDLE : ble_prf_types.h
- prf_is_cccd_value_valid() : ble_prf_utils.h
- prf_is_indication_enabled() : ble_prf_utils.h
- prf_is_notification_enabled() : ble_prf_utils.h
- prf_pack_char_pres_fmt() : ble_prf_utils.h
- prf_pack_date_time() : ble_prf_utils.h
- prf_unpack_char_pres_fmt() : ble_prf_utils.h
- prf_unpack_date_time() : ble_prf_utils.h
- PRIOR_RF_RX_PERFORMANCE : ble.h
- PRIOR_RF_RX_POWER : ble.h
- PROTOCOL_MODE : ble_lcp.h
- PSRAM_INIT_PARAMS_Default : app_graphics_ospi.h
- psram_reload_func_t : app_graphics_ospi.h
- PUBLIC : ble_iso.h
- PWM_ALIGNED_CENTER : gr55xx_hal_pwm.h
- PWM_ALIGNED_EDGE : gr55xx_hal_pwm.h
- PWM_DRIVEPOLARITY_NEGATIVE : gr55xx_hal_pwm.h
- PWM_DRIVEPOLARITY_POSITIVE : gr55xx_hal_pwm.h
- PWM_MODE_BREATH : gr55xx_hal_pwm.h
- PWM_MODE_FLICKER : gr55xx_hal_pwm.h
- PWM_PWR_ID : app_pwr_mgmt.h
- PWM_STOP_LVL_HIGH : gr55xx_hal_pwm.h
- PWM_STOP_LVL_LOW : gr55xx_hal_pwm.h
- pwr_before_sleep_func_t : gr55xx_pwr.h
- pwr_dev_check_func_t : gr55xx_pwr.h
- pwr_enter_sleep_check() : app_pwr_mgmt.h
- pwr_handler_t : gr55xx_hal_sleep_timer.h
- PWR_ID_MAX : app_pwr_mgmt.h
- pwr_id_t : app_pwr_mgmt.h
- PWR_MEM_POWER_FULL : gr55xx_hal_pwr.h
- PWR_MEM_POWER_OFF : gr55xx_hal_pwr.h
- PWR_MEM_POWER_RETENTION : gr55xx_hal_pwr.h
- pwr_mgmt_baseband_state_get() : gr55xx_pwr.h
- PWR_MGMT_BB_CHECK_FAIL : gr55xx_pwr.h
- pwr_mgmt_ble_wakeup() : gr55xx_pwr.h
- pwr_mgmt_check_ble_event() : gr55xx_pwr.h
- pwr_mgmt_check_ext_timer() : gr55xx_pwr.h
- pwr_mgmt_check_pend_irq() : gr55xx_pwr.h
- pwr_mgmt_dev_init() : gr55xx_pwr.h
- pwr_mgmt_dev_resume() : gr55xx_pwr.h
- pwr_mgmt_dev_state_t : gr55xx_pwr.h
- pwr_mgmt_dev_suspend() : gr55xx_pwr.h
- pwr_mgmt_disable_nvic_irq() : gr55xx_pwr.h
- pwr_mgmt_enable_nvic_irq() : gr55xx_pwr.h
- pwr_mgmt_get_wakeup_flag() : gr55xx_pwr.h
- pwr_mgmt_init() : gr55xx_pwr.h
- pwr_mgmt_load_context() : gr55xx_pwr.h
- pwr_mgmt_mem_ctl_set() : gr55xx_pwr.h
- PWR_MGMT_MODE_CHECK_FAIL : gr55xx_pwr.h
- pwr_mgmt_mode_get() : gr55xx_pwr.h
- pwr_mgmt_mode_set() : gr55xx_pwr.h
- pwr_mgmt_mode_t : gr55xx_pwr.h
- pwr_mgmt_notify_timer_event() : gr55xx_pwr.h
- pwr_mgmt_register_srpg_before_func() : gr55xx_pwr.h
- pwr_mgmt_register_trace_func() : gr55xx_pwr.h
- pwr_mgmt_save_context() : gr55xx_pwr.h
- pwr_mgmt_schedule() : gr55xx_pwr.h
- pwr_mgmt_set_callback() : gr55xx_pwr.h
- pwr_mgmt_set_wakeup_flag() : gr55xx_pwr.h
- pwr_mgmt_shutdown() : gr55xx_pwr.h
- pwr_mgmt_sleep() : gr55xx_pwr.h
- pwr_mgmt_ultra_sleep() : gr55xx_pwr.h
- pwr_mgmt_warm_boot() : platform_sdk.h
- pwr_mgmt_wfe_sleep() : gr55xx_pwr.h
- pwr_register_sleep_cb() : app_pwr_mgmt.h
- pwr_slp_elapsed_handler_t : gr55xx_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_NORMAL : gr55xx_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_RELOAD : gr55xx_hal_sleep_timer.h
- PWR_SLP_TIMER_MODE_SINGLE : gr55xx_hal_sleep_timer.h
- pwr_table : gr55xx_pwr.h
- PWR_TIMER_TYPE_AON_WDT : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_AON_WDT_TIMER : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_CAL_ALARM : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_CAL_TIMER : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_SLP_TIMER : gr55xx_hal_pwr.h
- pwr_unregister_sleep_cb() : app_pwr_mgmt.h
- pwr_wake_up_ind() : app_pwr_mgmt.h
- PWR_WKUP_COND_ALL : gr55xx_hal_pwr.h
- PWR_WKUP_COND_AON_WDT : gr55xx_hal_pwr.h
- PWR_WKUP_COND_AUSB : gr55xx_hal_pwr.h
- PWR_WKUP_COND_BLE : gr55xx_hal_pwr.h
- PWR_WKUP_COND_BLE_IRQ : gr55xx_hal_pwr.h
- PWR_WKUP_COND_BOD_FEDGE : gr55xx_hal_pwr.h
- PWR_WKUP_COND_CLDR : gr55xx_hal_pwr.h
- PWR_WKUP_COND_CLDR_TICK : gr55xx_hal_pwr.h
- PWR_WKUP_COND_DUSB : gr55xx_hal_pwr.h
- PWR_WKUP_COND_EXT : gr55xx_hal_pwr.h
- PWR_WKUP_COND_MSIO_COMP : gr55xx_hal_pwr.h
- PWR_WKUP_COND_TIMER : gr55xx_hal_pwr.h