Public Attributes | List of all members
gap_connless_cte_trans_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Set connectionless CTE transmit parameters. More...

`#include <ble_gapm.h>`

## Public Attributes
uint8_t | cte_len
| CTE length (8us unit, range 0x02 to 0x14). More...
uint8_t | cte_type
| CTE type (0: AOA | 1: AOD-1us | 2: AOD-2us) (. More...
uint8_t | cte_count
| CTE count (number of CTEs to transmit in each periodic advertising interval, range 0x01 to 0x10). More...
uint8_t | num_antenna
| The number of Antenna IDs in the pattern (range 0x02 to 0x4B). More...
uint8_t * | antenna_id
| List of Antenna IDs in the pattern. More...

## Detailed Description

Set connectionless CTE transmit parameters.

Definition at line 724 of file ble_gapm.h.

## Member Data Documentation

## ◆ antenna_id

uint8_t* gap_connless_cte_trans_param_t::antenna_id

List of Antenna IDs in the pattern.

Definition at line 730 of file ble_gapm.h.

## ◆ cte_count

uint8_t gap_connless_cte_trans_param_t::cte_count

CTE count (number of CTEs to transmit in each periodic advertising interval, range 0x01 to 0x10).

Definition at line 728 of file ble_gapm.h.

## ◆ cte_len

uint8_t gap_connless_cte_trans_param_t::cte_len

CTE length (8us unit, range 0x02 to 0x14).

Definition at line 726 of file ble_gapm.h.

## ◆ cte_type

uint8_t gap_connless_cte_trans_param_t::cte_type

CTE type (0: AOA | 1: AOD-1us | 2: AOD-2us) (.

See also
  enum gap_cte_type_t).

Definition at line 727 of file ble_gapm.h.

## ◆ num_antenna

uint8_t gap_connless_cte_trans_param_t::num_antenna

The number of Antenna IDs in the pattern (range 0x02 to 0x4B).

Definition at line 729 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h