Macros
FIFO Depth Defines
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for FIFO Depth Defines:

## Macros
#define | LL_QSPI_MAX_FIFO_DEPTH (32u)
| FIFO Depth for QSPI Master. More...
#define | LL_QSPI0_REG_RX_FIFO_DEPTH (16u)
| Receive FIFO Depth Of Register Mode for QSPI0 Master. More...
#define | LL_QSPI0_REG_TX_FIFO_DEPTH (16u)
| Transmit FIFO Depth Of Register Mode for QSPI0 Master. More...
#define | LL_QSPI0_XIP_RX_FIFO_DEPTH (32u)
| Receive FIFO Depth Of XIP Mode for QSPI0 Master. More...
#define | LL_QSPI0_XIP_TX_FIFO_DEPTH (16u)
| Transmit FIFO Depth Of XIP Mode for QSPI0 Master. More...
#define | LL_QSPI1_REG_RX_FIFO_DEPTH (32u)
| Receive FIFO Depth Of Register Mode for QSPI1 Master. More...
#define | LL_QSPI1_REG_TX_FIFO_DEPTH (32u)
| Transmit FIFO Depth Of Register Mode for QSPI1 Master. More...
#define | LL_QSPI1_XIP_RX_FIFO_DEPTH (32u)
| Receive FIFO Depth Of XIP Mode for QSPI1 Master. More...
#define | LL_QSPI1_XIP_TX_FIFO_DEPTH (32u)
| Transmit FIFO Depth Of XIP Mode for QSPI1 Master. More...
#define | LL_QSPI2_REG_RX_FIFO_DEPTH (16u)
| Receive FIFO Depth Of Register Mode for QSPI2 Master. More...
#define | LL_QSPI2_REG_TX_FIFO_DEPTH (32u)
| Transmit FIFO Depth Of Register Mode for QSPI2 Master. More...
#define | LL_QSPI2_XIP_RX_FIFO_DEPTH (16u)
| Receive FIFO Depth Of XIP Mode for QSPI2 Master. More...
#define | LL_QSPI2_XIP_TX_FIFO_DEPTH (16u)
| Transmit FIFO Depth Of XIP Mode for QSPI2 Master. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI0_REG_RX_FIFO_DEPTH

#define LL_QSPI0_REG_RX_FIFO_DEPTH (16u)

Receive FIFO Depth Of Register Mode for QSPI0 Master.

Definition at line 285 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI0_REG_TX_FIFO_DEPTH

#define LL_QSPI0_REG_TX_FIFO_DEPTH (16u)

Transmit FIFO Depth Of Register Mode for QSPI0 Master.

Definition at line 286 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI0_XIP_RX_FIFO_DEPTH

#define LL_QSPI0_XIP_RX_FIFO_DEPTH (32u)

Receive FIFO Depth Of XIP Mode for QSPI0 Master.

Definition at line 287 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI0_XIP_TX_FIFO_DEPTH

#define LL_QSPI0_XIP_TX_FIFO_DEPTH (16u)

Transmit FIFO Depth Of XIP Mode for QSPI0 Master.

Definition at line 288 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI1_REG_RX_FIFO_DEPTH

#define LL_QSPI1_REG_RX_FIFO_DEPTH (32u)

Receive FIFO Depth Of Register Mode for QSPI1 Master.

Definition at line 290 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI1_REG_TX_FIFO_DEPTH

#define LL_QSPI1_REG_TX_FIFO_DEPTH (32u)

Transmit FIFO Depth Of Register Mode for QSPI1 Master.

Definition at line 291 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI1_XIP_RX_FIFO_DEPTH

#define LL_QSPI1_XIP_RX_FIFO_DEPTH (32u)

Receive FIFO Depth Of XIP Mode for QSPI1 Master.

Definition at line 292 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI1_XIP_TX_FIFO_DEPTH

#define LL_QSPI1_XIP_TX_FIFO_DEPTH (32u)

Transmit FIFO Depth Of XIP Mode for QSPI1 Master.

Definition at line 293 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI2_REG_RX_FIFO_DEPTH

#define LL_QSPI2_REG_RX_FIFO_DEPTH (16u)

Receive FIFO Depth Of Register Mode for QSPI2 Master.

Definition at line 295 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI2_REG_TX_FIFO_DEPTH

#define LL_QSPI2_REG_TX_FIFO_DEPTH (32u)

Transmit FIFO Depth Of Register Mode for QSPI2 Master.

Definition at line 296 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI2_XIP_RX_FIFO_DEPTH

#define LL_QSPI2_XIP_RX_FIFO_DEPTH (16u)

Receive FIFO Depth Of XIP Mode for QSPI2 Master.

Definition at line 297 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI2_XIP_TX_FIFO_DEPTH

#define LL_QSPI2_XIP_TX_FIFO_DEPTH (16u)

Transmit FIFO Depth Of XIP Mode for QSPI2 Master.

Definition at line 298 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_MAX_FIFO_DEPTH

#define LL_QSPI_MAX_FIFO_DEPTH (32u)

FIFO Depth for QSPI Master.

Definition at line 283 of file gr55xx_ll_qspi.h.