Macros
Instruction Size For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

More...

Collaboration diagram for Instruction Size For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_INSTSIZE_0BIT 0x0 /* no instruction */
#define | LL_QSPI_CONCURRENT_XIP_INSTSIZE_4BIT 0x1 /* instruction size equals 4bits */
#define | LL_QSPI_CONCURRENT_XIP_INSTSIZE_8BIT 0x2 /* instruction size equals 8bits */
#define | LL_QSPI_CONCURRENT_XIP_INSTSIZE_16BIT 0x3 /* instruction size equals 16bits */

## Detailed Description

Instruction size for concurrent xip mode

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_INSTSIZE_0BIT

#define LL_QSPI_CONCURRENT_XIP_INSTSIZE_0BIT 0x0 /* no instruction */

Definition at line 600 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INSTSIZE_16BIT

#define LL_QSPI_CONCURRENT_XIP_INSTSIZE_16BIT 0x3 /* instruction size equals 16bits */

Definition at line 603 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INSTSIZE_4BIT

#define LL_QSPI_CONCURRENT_XIP_INSTSIZE_4BIT 0x1 /* instruction size equals 4bits */

Definition at line 601 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INSTSIZE_8BIT

#define LL_QSPI_CONCURRENT_XIP_INSTSIZE_8BIT 0x2 /* instruction size equals 8bits */

Definition at line 602 of file gr55xx_ll_qspi.h.