Public Attributes | List of all members
_dspi_command_t Struct Reference
Peripheral Driver » HAL Driver » DSPI » Structures » DSPI command

DSPI command Structure definition. More...

`#include <gr55xx_hal_dspi.h>`

## Public Attributes
uint32_t | instruction
| Specifies the Instruction to be sent. More...
uint32_t | instruction_size
| Specifies the Instruction Size. More...
uint32_t | data_size
| Specifies the DSPI data width. More...
uint32_t | length
| Specifies the number of data to transfer. More...

## Detailed Description

DSPI command Structure definition.

Definition at line 153 of file gr55xx_hal_dspi.h.

## Member Data Documentation

## ◆ data_size

uint32_t _dspi_command_t::data_size

Specifies the DSPI data width.

This parameter can be a value of Data Width.

Definition at line 161 of file gr55xx_hal_dspi.h.

## ◆ instruction

uint32_t _dspi_command_t::instruction

Specifies the Instruction to be sent.

This parameter can be a value (8-bit, 16bit, 32 bit).

Definition at line 155 of file gr55xx_hal_dspi.h.

## ◆ instruction_size

uint32_t _dspi_command_t::instruction_size

Specifies the Instruction Size.

This parameter can be a value of DSPI Instruction Size.

Definition at line 158 of file gr55xx_hal_dspi.h.

## ◆ length

uint32_t _dspi_command_t::length

Specifies the number of data to transfer.

(This is the number of bytes). This parameter can be any value between 0 and 0xFFFFFFFF (0 means undefined length until end of memory).

Definition at line 164 of file gr55xx_hal_dspi.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_dspi.h