### - g -

- GAP_PHY_ANY : ble_gapc.h
- GAP_PHY_LE_1MBPS : ble_gapc.h
- GAP_PHY_LE_2MBPS : ble_gapc.h
- GAP_PHY_LE_CODED : ble_gapc.h
- GDC_ACCESS_TYPE_ASYNC : app_graphics_dc.h
- GDC_ACCESS_TYPE_SYNC : app_graphics_dc.h
- GDC_CLOCK_FREQ_12MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_24MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_3MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_48MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_6MHz : app_graphics_dc.h
- GDC_CLOCK_MODE_0 : app_graphics_dc.h
- GDC_CLOCK_MODE_1 : app_graphics_dc.h
- GDC_CLOCK_MODE_2 : app_graphics_dc.h
- GDC_CLOCK_MODE_3 : app_graphics_dc.h
- GDC_DATA_FORMAT_ABGR8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_ARGB8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_BGRA8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGB24 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGB565 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGBA8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC4 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC6 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC6A : app_graphics_dc.h
- GDC_DSPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_08BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_16BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_24BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_NONE : app_graphics_dc.h
- GDC_FRAME_RES_ASYNC_WAIT : app_graphics_dc.h
- GDC_FRAME_RES_FAIL : app_graphics_dc.h
- GDC_FRAME_RES_SUCCESS : app_graphics_dc.h
- GDC_FRAME_RES_UNSUPPORT : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB888_OPT1 : app_graphics_dc.h
- GDC_MIPICFG_QSPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_QSPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_SPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_SPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MODE_DSPI : app_graphics_dc.h
- GDC_MODE_QSPI : app_graphics_dc.h
- GDC_MODE_SPI : app_graphics_dc.h
- GDC_ONE_LAYER_MODE : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_16 : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_24 : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_NOT_SUPPORT : app_graphics_dc.h
- GDC_POWER_STATE_ACTIVE : app_graphics_dc.h
- GDC_POWER_STATE_SLEEP : app_graphics_dc.h
- GDC_QSPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_QSPI_FRAME_TIMING_1 : app_graphics_dc.h
- GDC_SPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_TCSU_CYCLE_0 : app_graphics_dc.h
- GDC_TCSU_CYCLE_1 : app_graphics_dc.h
- GDC_TCSU_CYCLE_2 : app_graphics_dc.h
- GDC_TCSU_CYCLE_3 : app_graphics_dc.h
- GDC_TCSU_CYCLE_4 : app_graphics_dc.h
- GDC_TWO_LAYER_MODE : app_graphics_dc.h
- GPIO_PIN_RESET : gr55xx_hal_gpio.h
- GPIO_PIN_SET : gr55xx_hal_gpio.h
- GPU_POWER_STATE_ACTIVE : app_graphics_gpu.h
- GPU_POWER_STATE_SLEEP : app_graphics_gpu.h
- GUS_C_EVT_DISCOVERY_COMPLETE : gus_c.h
- GUS_C_EVT_DISCOVERY_FAIL : gus_c.h
- GUS_C_EVT_FLOW_CTRL_NTF_SET_SUCCESS : gus_c.h
- GUS_C_EVT_INVALID : gus_c.h
- GUS_C_EVT_PEER_DATA_RECEIVE : gus_c.h
- GUS_C_EVT_RX_FLOW_UPDATE_CPLT : gus_c.h
- GUS_C_EVT_TX_CPLT : gus_c.h
- GUS_C_EVT_TX_FLOW_OFF : gus_c.h
- GUS_C_EVT_TX_FLOW_ON : gus_c.h
- GUS_C_EVT_TX_NTF_SET_SUCCESS : gus_c.h
- GUS_C_EVT_WRITE_OP_ERR : gus_c.h
- GUS_C_FLOW_CTRL_STATE_OFF : gus_c.h
- GUS_C_FLOW_CTRL_STATE_ON : gus_c.h
- GUS_EVT_FLOW_CTRL_DISABLE : gus.h
- GUS_EVT_FLOW_CTRL_ENABLE : gus.h
- GUS_EVT_INVALID : gus.h
- GUS_EVT_RX_DATA_RECEIVED : gus.h
- GUS_EVT_TX_DATA_SENT : gus.h
- GUS_EVT_TX_FLOW_OFF : gus.h
- GUS_EVT_TX_FLOW_ON : gus.h
- GUS_EVT_TX_PORT_CLOSED : gus.h
- GUS_EVT_TX_PORT_OPENED : gus.h
- GUS_FLOW_CTRL_STATE_OFF : gus.h
- GUS_FLOW_CTRL_STATE_ON : gus.h