Macros
Frame Format For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

Frame format for concurrent xip mode. More...

Collaboration diagram for Frame Format For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_FRF_RSVD 0x0
| SPI Frame format : Reserved. More...
#define | LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI 0x1
| SPI Frame format : DUAL More...
#define | LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI 0x2
| SPI Frame format : QUAD More...
#define | LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI 0x3
| SPI Frame format : OCTAL More...

## Detailed Description

Frame format for concurrent xip mode.

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_DUAL_SPI 0x1

SPI Frame format : DUAL

Definition at line 642 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_OCTAL_SPI 0x3

SPI Frame format : OCTAL

Definition at line 644 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI

#define LL_QSPI_CONCURRENT_XIP_FRF_QUAD_SPI 0x2

SPI Frame format : QUAD

Definition at line 643 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_FRF_RSVD

#define LL_QSPI_CONCURRENT_XIP_FRF_RSVD 0x0

SPI Frame format : Reserved.

Definition at line 641 of file gr55xx_ll_qspi.h.