Macros
BLOCK Mode for LLP
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for BLOCK Mode for LLP:

## Macros
#define | QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_0 0u
| This is Loop Block Mode, inst & addr in the head of each block, data are following insta & addr in the same block. More...
#define | QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_1 1u
| This is Crossed Block Mode, inst & addr in the first block, data in the second block, then inst & addr block, then data block again, and repeat till the end. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_0

#define QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_0 0u

This is Loop Block Mode, inst & addr in the head of each block, data are following insta & addr in the same block.

Definition at line 698 of file gr55xx_hal_qspi.h.

## ◆ QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_1

#define QSPI_PSRAM_LINKED_BLOCK_DATA_MODE_1 1u

This is Crossed Block Mode, inst & addr in the first block, data in the second block, then inst & addr block, then data block again, and repeat till the end.

Definition at line 701 of file gr55xx_hal_qspi.h.