Macros
RX/TX FIFO depth
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants
Collaboration diagram for RX/TX FIFO depth:

## Macros
#define | LL_I2S_FIFO_DEPTH_2 (0UL)
| FIFO depth is 2 . More...
#define | LL_I2S_FIFO_DEPTH_4 (1UL)
| FIFO depth is 4 . More...
#define | LL_I2S_FIFO_DEPTH_8 (2UL)
| FIFO depth is 8 . More...
#define | LL_I2S_FIFO_DEPTH_16 (3UL)
| FIFO depth is 16. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_FIFO_DEPTH_16

#define LL_I2S_FIFO_DEPTH_16 (3UL)

FIFO depth is 16.

Definition at line 238 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_FIFO_DEPTH_2

#define LL_I2S_FIFO_DEPTH_2 (0UL)

FIFO depth is 2 .

Definition at line 235 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_FIFO_DEPTH_4

#define LL_I2S_FIFO_DEPTH_4 (1UL)

FIFO depth is 4 .

Definition at line 236 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_FIFO_DEPTH_8

#define LL_I2S_FIFO_DEPTH_8 (2UL)

FIFO depth is 8 .

Definition at line 237 of file gr55xx_ll_i2s.h.