Macros
Characteristics Mask
BLE Services » Phone Alert Status Service (PASS) » Defines

Bit masks for the initialization of pass_init_t::char_mask. More...

Collaboration diagram for Characteristics Mask:

## Macros
#define | PASS_CHAR_MANDATORY 0x003f
| Bit mask for mandatory characteristic in PASS. More...
#define | PASS_CHAR_RING_CTRL_PT_SUP 0x0180
| Bit mask for Ringer Control Point characteristic in PASS. More...
#define | PASS_CHAR_FULL 0x01ff
| Bit mask of the full characteristic. More...

## Detailed Description

Bit masks for the initialization of pass_init_t::char_mask.

## Macro Definition Documentation

## ◆ PASS_CHAR_FULL

#define PASS_CHAR_FULL 0x01ff

Bit mask of the full characteristic.

Definition at line 80 of file pass.h.

## ◆ PASS_CHAR_MANDATORY

#define PASS_CHAR_MANDATORY 0x003f

Bit mask for mandatory characteristic in PASS.

Definition at line 78 of file pass.h.

## ◆ PASS_CHAR_RING_CTRL_PT_SUP

#define PASS_CHAR_RING_CTRL_PT_SUP 0x0180

Bit mask for Ringer Control Point characteristic in PASS.

Definition at line 79 of file pass.h.